# Installing SD Card

SD card is installed in the main board of the printer unit using the following procedure.

IMPORTANT
###### When using the "Encrypted Secured Print" function whose security is reinforced for data communication and stored data You need to install "Encrypted Secured Print Driver Add-in." For details on the installation procedure, see "Readme.txt" in the supplied CD-ROM.
| We recommend that an encrypted secured print be used when printing secured print jobs.
###### Before installing SD card If the SD card is write-protected, release the protection, and then insert the card.

1
Turn the printer OFF, then disconnect the cables or cords from the printer.

| Shut down the printer before turning it OFF. For details on the procedure for shutting down the printer, see "Turning the Printer ON/OFF."

##### <How to disconnect the cable or cord>

USB cable* | (2) Turn the computer OFF. (3) Disconnect the cable from the printer.
LAN cable* | (4) Disconnect the cable from the printer.
Power cord | (5) Disconnect the power plug from the AC power outlet. (6) Disconnect the cord from the printer.

* | Whether the cable is connected or not varies depending on your environment.

2
Remove the right cover.

(1) | While holding the tab (A), open the cover a little.
(2) | Remove the cover in the direction of the arrow.

3
Install SD card.
Insert the SD card in the SD card slot until it clicks.
4
Attach the right cover.

(1) | Attach the right cover.
(2) | Close the cover.

5
Hard reset or restart the printer.
If <Formatting SD Card?> appears in the display after the printer starts, the SD card is being formatted.
Wait for a moment until the format is completed.

IMPORTANT
###### If <Formatting SD Card?> does not appear in the display Perform [Format] in [SD Card Maintenance] in the common Setup menu. "[Setup] Menu ([User Maintenance] Options)"

6
Connect all the interface cables.

NOTE
###### Setting after the SD card is installed Perform the following procedure after the SD card is installed.
(1) | Display the [Device Settings] sheet in the printer driver. For details on the procedure for displaying the sheet, see "Setting the Printer Options."
(2) | Click [Get Device Status]. If you cannot obtain the status of the optional accessories automatically, select the [SD Card Installed] check box.
For details on the procedure for Macintosh, see "Setting the Printer Options."

Next, perform the following procedures.
| ###### If you install the printer and SD card at the same time
1 | Connect the power cord. | "Connecting the Power Cord"
2 | Specifying the printer's initial settings. | "Turning the Power On and Specifying a Language and Time"
Specifying a type of printer driver. | "Specifying a Type of Printer Driver"
3 | Load paper. | "Loading Paper in the Drawer" "Loading Paper in the Multi-purpose Tray"
4 | Connecting to a computer. | "Connecting to a Computer"
5 | Install the printer driver. | "For Windows" "For Macintosh"
6 | Check the printing operation. | Check the operations by Test Page in Windows. "Basic Operations/Various Information for Windows"
7 | Checking the ROM Installation. (Only when installing ROM) | "Checking the ROM Installation"
Checking the SD Card Installation. | "Checking the SD Card Installation"
8 | Specify the settings for the ROM module as needed. | Specify the settings in the menu functions. "[Setup] Menu ([PS] Options)" For details on the settings for the bar code fonts, see "Bar Code Printing Guide" included in the User Manual CD-ROM.
| ###### If you installed SD card afterward (If you are using the printer already)
1 | Connect the cables and cords. | Connect the removed cables and cords again.
2 | Checking the ROM Installation. (Only when installing ROM) | "Checking the ROM Installation"
Checking the SD Card Installation. | "Checking the SD Card Installation"
3 | Specify the settings for the ROM module as needed. | Specify the settings in the menu functions. "[Setup] Menu ([PS] Options)" For details on the settings for the bar code fonts, see "Bar Code Printing Guide" included in the User Manual CD-ROM.

0258-0RU