# [Setup] Menu ([Layout] Options)

NOTE
###### Table description Bold values in the table indicate the default settings. ###### About the icon
: | The settings for the printer driver are prioritized for this item.

Setting Item | Setting Value | Setting
[Copies] | 1 to 9999 | Specifies the number of copies to be printed. The printer prints the specified number of copies.
[Offset Y]/[Offset X] | -50.0 to 0.0 to +50.0 (mm) | Adjusts the printing position in the vertical direction (Y) or the horizontal direction (X) by the specified value. "Adjusting the Printing Position for All the Jobs"
[Binding Location] | [Long Edge], [Short Edge] | Specifies which edge of the paper, the long edge or short edge, is to be bound. When performing 2-sided printing, the printer adjusts the binding location automatically according to the paper surface. If [Long Edge] is specified, the binding location is created on the long edge of the paper. If [Short Edge] is specified, the binding location is created on the short edge of the paper.
[Gutter] | -50.0 to 0.0 to +50.0 (mm) | Specifies the gutter width for printing with the binding location created. A gutter is created with the image shifted by the specified value. You can shift the image in the "+" direction with a positive value and in the "-" direction with a negative value.
[Alternative Method] | [Off], [On] | If this item is set to [On] and if the last page for the 2-sided printing is 1-sided printing, 1-sided printing is applied to the last page. (Printing can be performed faster than normal 2-sided printing.) However, when performing 2-sided printing on punched paper or previously printed paper, the orientation or printing surface of the last page may differ from other pages. In this case, specify [Off].

0258-08U