# Specifying the Setting for Startup Waiting Time

Specify the setting for startup waiting time using either of the following methods.
"Performing the Configuration Using the Printer's Control Panel"
Specify the setting for startup waiting time using the control panel while checking the display on the printer.
"Changing the Settings Using Web Browser (Remote UI)"
Specify the setting for startup waiting time by accessing the printer from a Web browser via the network.

| Normally, you do not need to change the setting for startup waiting time (the time from when you turn the printer ON to when the printer starts communication). Specify the setting for the startup waiting time only when the printer cannot be connected to the network.

NOTE
###### If this printer is connected to a switching hub etc. The printer may not be able to be connected to the network even when the network settings are correct. This is because the printer and hub cannot communicate each other immediately after this printer is connected to the hub due to a spanning tree process. In this case, it is necessary to set a delay before establishing the network connection with the printer using this setting. For details on the functions of a switching hub, contact the manufacturer of the switching hub. ###### Changing the settings using FTP Client You can also specify the setting for startup waiting time using FTP Client. "FTP Client"

0258-06F