# Automatically Performing Calibration Immediately after the Printer Is Turned ON

You can set the timing for performing calibration when the self-diagnostic immediately after the printer is turned ON determines that calibration is necessary.
1
Press [ ] (: Online).

→ | The Online indicator goes off, allowing you to specify the settings on the control panel.

2
Press [ ] (: Settings).
3
Select [User Maintenance] using [ ] and [ ], and then press [OK].
4
Select [First Calibration] using [ ] and [ ], and then press [OK].
5
Select [Color Mismatch Corr.] using [ ] and [ ], and then press [OK].
6
Set the [Color Mismatch Corr.] operation that is run immediately after the printer is turned ON.
Select [After Jobs] or [Immediately] with [ ] or [ ], and press [OK].

After Jobs | It runs color mismatch adjustment after the first print job after the printer is turned ON is completed.
Immediately | Print color mismatch is adjusted immediately after the printer is turned ON. If color mismatch adjustment is run immediately after the printer is turned ON, it will take some time before it is possible to print.

7
Select [Density Control] using [ ] and [ ], and then press [OK].
8
Set the [Density Control] operation that is run immediately after the printer is turned ON.
Select [Off], [After Jobs] or [Immediately] with [] or [], and press [OK].

Off | If the printer is used in an environment with wide temperature variation, it may run density control.
After Jobs | It runs density control after the first print job after the printer is turned ON is completed.
Immediately | It runs density control immediately after the printer is turned ON. If density control is run immediately after the printer is turned ON, it will take some time before it is possible to print.

→ | The setting for [First Calibration] is changed.

0258-0LL