# The Printing Position Is Skewed

Perform one of the following solutions according to the cause.

#### <Cause 1> [Gutter] is specified.

Solution | Perform the following procedure in the printer driver.
1. | Display the [Finishing] sheet.
2. | Click [Gutter].
3. | Set [Gutter] to "0."
You can specify the same setting from the printer's control panel. "[Setup] Menu ([Layout] Options)"

#### <Cause 2> [Offset Y] and [Offset X] are specified.

Solution | Set [Offset Y] and [Offset X] to "0." "Adjusting the Printing Position for All the Jobs"

#### <Cause 3> "Top Margin" and "Paper Position" in the application are not specified properly.

Solution | Specify the settings for "Top Margin" and "Paper Position" in the application properly. See the instruction manual supplied with the application.

#### <Cause 4> The printing position is adjusted in [Adj. Start Position].

Solution | Adjust the printing position to an appropriate value in [Adj. Start Position]. "Adjusting the Printing Position for Each Paper Source"

0258-0E3