# Confirming the Supplied Accessories and Checking the Installation Site

## Confirming the Supplied Accessories

Make sure that all the supplied accessories are contained in the box before installing the printer.
If an item is missing or damaged, please contact your local authorized Canon dealer.

IMPORTANT
###### Download the printer driver for Macintosh from the Canon Web site The supplied CD-ROM does not include the printer driver for Macintosh. Download the printer driver for Macintosh that supports this printer from the Canon Web site (http://www.canon.com/). If you cannot find the printer driver for Macintosh that supports this printer on the Canon Web site, contact your local authorized Canon dealer.

NOTE
###### About interface cables This printer does not come with an interface cable. Have an appropriate one available for the computer you are using or the connecting method. Use a USB cable with the following symbol.

#### About the Supplied Manuals

The manuals supplied with this printer consist of the following. Read these manuals according to your purpose and make full use of this printer.

Manual Name | Contents
Quick Setup Guide | Explains the procedure for installing the printer.
e-Manual | Explains all the operations of this printer, such as how to use the printer and troubleshooting. (The contents of "Quick Setup Guide" are also included.)
Getting Started Guide | This is the simple manual (PDF format) written in the following languages. Arabic, Bulgarian, Croatian, Estonian, Greek, Latvian, Lithuanian, Persian, Romanian, Slovakian, Slovenian, Ukrainian

To view the manual in PDF format, Adobe Reader/Adobe Acrobat Reader is required.
If Adobe Reader/Adobe Acrobat Reader is not installed on your system, download it from the Adobe Systems Incorporated Web site.

## Checking the Installation Site

In order to use this printer in a safe and trouble-free manner, install the printer in a place that fulfills the following conditions.

###### Temperature and Humidity Conditions

Temperature range | 10 to 30°C (50 to 86°F)
Humidity range | 20 to 80% RH (no condensation)

###### Power Supply Requirements

220 to 240 V (±10%), 50/60 Hz (±2 Hz)

###### Installation Requirements

A location with sufficient space

|  | Refer to the following dimensions of each part and ensure the installation space.

A location with good ventilation
A location with a flat, even surface
A location able to fully support the weight of the printer
0258-023