# Setting TTLS/PEAP Authentication Information

Set authentication information for using TTLS or PEAP with IEEE802.1X authentication.
TTLS and PEAP perform mutual authentication using the authentication server's certificate and the user name and password set in the printer.

IMPORTANT
###### In order to set a user name and password You need to set up the SSL encryption communication function in advance. Setting the SSL Encryption Communication Function

1
Start the Remote UI, and then log in as Administrator.
Starting the Remote UI
2
Click [Settings/Registration].
3
Select [Network] from the [Preferences] menu.
4
Click [IEEE802.1X Settings].
5
Click [Edit...].
6
Enter the login name.
Up to 24 alphanumeric characters can be entered.
7
Select the [Use TTLS] or [Use PEAP] check box.

###### When using TTLS

Select the internal TTLS authentication method.
(1) Select the [MSCHAPv2] or [PAP] check box.
8
Click [Change User Name/Password...].

###### When using the log in name entered in Step 6 as the user name

Select the [Use Login Name as User Name] check box.
9
Enter user name.
Up to 24 alphanumeric characters can be entered.
10
Enter password.

(1) | Select the [Change Password] check box.
(2) | Enter password. You can enter up to 24 characters.
(3) | Enter the same password in the [Confirm] field.
(4) | Click [OK].

11
Select the [Use IEEE802.1X] check box.

If a Message Appears A message will be displayed if there is anything wrong with the settings. See Steps 6 to 10, and check the settings.

12
Click [OK].
13
Perform a hard reset or restart the printer.

→ | After performing a hard reset or restarting the printer, the settings are effective.

NOTE
###### To perform a hard reset You can perform a hard reset using the following procedure.
1. | Click [Settings/Registration].
2. | Select [Device Control] from the [Output/Control] menu.
3. | Select [Hard Reset], then click [Execute].

0258-0L8