# Printing on Labels

#### Confirming usable labels

This printer can use the following sizes of labels.

Standard sizes | A4, B5, A5, Legal, Letter, Executive, Statement, and Foolscap
Custom paper sizes | Width 76.2 to 215.9 mm, Length 127.0 to 355.6 mm*

* | If you are using the UFR II printer driver, you can load custom size paper that is 127.0 to 215.9 mm wide and 127.0 to 215.9 mm long also in landscape orientation.

| Using the following types of labels may result in paper jams that are difficult to clear or may result in damage to the printer. Peeled labels or partly used labels Coated labels that are easily peeled off from the backing sheet Labels with uneven adhesive

#### Loading labels

Labels can be loaded in the drawer or the Multi-purpose tray.
"Loading Paper in the Drawer"
"Loading Paper in the Multi-purpose Tray"

###### <Precautions when loading labels>

Fan the labels thoroughly, and then align the edges before loading them. If they are not fanned enough, multiple sheets of paper may be fed at once, causing paper jams.
Take care not to mark or stain the printing surface of the labels with fingerprints, dust, or oil. This may result in poor print quality.

#### Printing from an application

After loading labels, perform printing.
"Configuring the Printer Driver and Printing"

| The print speed may drop when printing on labels.

0258-040