# Setting the IP Address (IP v. 4)

There are the following three methods for setting the IP address.

#### Setting the IP Address Using the Printer's Control Panel
| Set the IP address using the control panel while checking the display on the printer.
#### Setting the IP Address Using the ARP/PING Commands
| Set the IP address using the ARP/PING command in Command Prompt.
#### Setting the IP Address Using NetSpot Device Installer
| Set the IP address using NetSpot Device Installer in the supplied CD-ROM.

IMPORTANT
###### When setting the IP Address using the ARP/PING command or NetSpot Device Installer The MAC address of the printer is required. For details on the procedure for checking the MAC address, see "Checking the MAC Address." ###### Before setting the IP address Make sure that the printer is connected to the network and the printer is ON.

NOTE
###### If you changed the IP address after installing the printer driver Specify the port to be used again in the printer driver. "Configuring a Computer that Performs Printing"

0258-06Y