# Printer Specifications

## Hardware Specifications

Type | Desktop Page Printer
Printing System | Semiconductor laser + xerographic system
Toner fixing system | On-demand fixing system
Resolution | 600 dpi
Printing speed (Plain paper (60 to 90 g/m²), when printing A4 size paper continuously) | Black and white printing: 20 pages/minute Color printing: 20 pages/minute
| The print speed may drop depending on the paper settings for the size, type, orientation, and number of copies.
Warm up time (Time from power on to printer ready) | 31 seconds or less
| May vary depending on the usage conditions, such as the availability of the optional accessories and installation environment.
Recovery time (Time from the sleep mode to printer ready) | 8 seconds when the printer is in Sleep Mode 1 (the Printer Sleep mode) 9 seconds when the printer is in Sleep Mode 2 (the Deep Sleep mode)*
* | It is the default setting. For details on [Sleep Mode], see "Sleep Mode."
| May vary depending on the output environment.
First print time (When performing 1-sided printing on A4 size paper and outputting face-down) | Black and white printing: 16 seconds or less Color printing: 16 seconds or less
| May vary depending on the output environment.
Paper size | Drawer 1/Drawer 2 (Optional) Standard sizes: A4, B5, A5, Legal, Letter, Executive, Statement, Foolscap, Envelope DL, Envelope COM-10, Envelope ISO-C5, and Envelope ISO-B5 Custom paper sizes *1: Width 100.0 to 215.9 mm, Length 148.0 to 355.6 mm
| If you are using the UFR II printer driver, you can load custom size paper that is 148.0 to 215.9 mm wide and 148.0 to 215.9 mm long also in landscape orientation.
Multi-purpose tray Standard sizes: A4, B5, A5, Legal, Letter, Executive, Statement, Foolscap, Index Card, Envelope DL, Envelope COM-10, Envelope ISO-C5, Envelope ISO-B5, and Envelope Monarch Custom paper sizes *1: Width 76.2 to 215.9 mm, Length 127.0 to 355.6 mm
| If you are using the UFR II printer driver, you can load custom size paper that is 127.0 to 215.9 mm wide and 127.0 to 215.9 mm long also in landscape orientation.
*1 | Width must not be greater than length (height).
Paper capacity | Drawer 1/Drawer 2 (Optional): Approx. 250 sheets Multi-purpose tray: Approx. 50 sheets
2-sided printing | A4, B5, Legal, Letter, Executive, Foolscap
Paper output | Face-down
Output capacity | Approx. 125 sheets
Noise (Declared noise emission in accordance with ISO 9296) | LwAd (declared A-weighted sound power level (1 B = 10 dB)) During standby: 43 dB or less During operation: 6.7 B or less LpAm (declared A-weighted sound pressure level (bystander position)) During standby: 24 dB During operation: 52 dB
Operating environment (Printer unit only) | Operating environment Temperature range: 10 to 30°C (50 to 86°F) Humidity range: 20 to 80% RH (no condensation)
Power supply | 220 to 240 V (±10%), 50/60 Hz (±2 Hz)
Power consumption (at 20°C (68°F)) | Maximum: 950 W or less Average during operation: Approx. 405 W Average during standby: Approx. 23 W Average during Printer Sleep Mode (Sleep Mode 1): Approx. 7.5 W Average during Deep Sleep Mode (Sleep Mode 2): Approx. 1 W* When the main power switch is turned OFF: 0.1 W or less
* | It is the default setting. For details on [Sleep Mode], see "Sleep Mode."
| Even if the power of the printer is turned OFF, power is consumed only slightly while the power plug is inserted into the AC power outlet. To cut the power consumption completely, unplug the power plug from the AC power outlet.
Consumables | Canon Cartridge 718 Yellow Canon Cartridge 718 Magenta Canon Cartridge 718 Cyan Canon Cartridge 718 Black
| For details on the yield, see "Replacement Timing" in "Consumables."
Weight | Printer unit and included parts Printer unit (excluding the toner cartridge): Approx. 22.4 kg Toner cartridge (each): Approx. 0.7 kg Consumables and optional accessories Toner cartridge (each) (Canon Genuine Cartridge): Approx. 0.7 kg Paper Feeder Unit PF-701 (including the drawer): Approx. 4 kg

## Controller Specifications

CPU | 528 MHz + 264 MHz
Memory (RAM) capacity | 768 MB
Host interface | LBP7680Cx USB interface: Hi-Speed USB (1) USB (1 front and 1 back) Network interface: Shared 10BASE-T/100BASE-TX/1000BASE-T (RJ-45) Full duplex/Half duplex LBP7660Cdn USB interface: Hi-Speed USB (1) USB (1) Network interface: Shared 10BASE-T/100BASE-TX/1000BASE-T (RJ-45) Full duplex/Half duplex
User interface | LCD: 132 x 65 dots F-STN liquid crystal display LED indicator: 8 Operation key: 12 (LBP7680Cx) / 10 (LBP7660Cdn)
ROM slot | 1
SD card slot (LBP7680Cx only) | 1

## Software Specifications

Built-in control command | LBP7680Cx PCL 5c, PCL 6, PostScript 3 emulation, and UFR II LBP7660Cdn PCL 5c, PCL 6, and UFR II
Built-in fonts | LBP7680Cx PCL: 93 Scalable fonts, 10 Bitmap fonts PS: 136 standard fonts LBP7660Cdn PCL: 45 Scalable fonts, 10 Bitmap fonts
Printable area | PCL 5c/PCL 6: Data cannot be printed within a 4.2 mm margin (10 mm margin for envelopes) on all sides of the paper. UFR II/PS (PS for LBP7660Cdn is an option.): Data cannot be printed within a 5 mm (10 mm for envelopes) margin on all sides of the paper.
| For details, see "Printable Area."
Network interface | Supported protocol TCP/IP (Frame type: Ethernet II) AppleTalk NetWare (LBP7680Cx only) SMB (option) (LBP7680Cx only) Print application LPD RAW IPP/IPPS FTP WSD

0258-011