# Network Setting Items

You can change the network settings using various methods.
Network Setting Items
Software That Can Be Used for the Network Settings

## Network Setting Items

The setting items you can change using NetSpot Device Installer, FTP Client, or the control panel on the printer are as follows.

NOTE
###### The settings that you cannot specify using FTP Client, NetSpot Device Installer, or the control panel on the printer Specify them using a Web browser (Remote UI). (However, you cannot specify the settings with even using the Remote UI.) ###### About the item names In the following table, the characters shown in parentheses are exclusively for FTP Client. For example, "[IP Address] (INT_ADDR)" is displayed differently as follows, depending on the application.
Web browser (Remote UI): | [IP Address]
NetSpot Device Installer: | [IP Address]
config file of FTP Client: | [INT_ADDR]
Control Panel: | [IP Address]

#### General Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[System Manager Password] (ROOT_PWD) | Up to 16 characters | (Blank) |  |  |
[System Manager] (SYS_CONTACT) | Up to 32 characters | (Blank) |  |  |
[Device Name] (DEVICE_NAME) | Up to 32 characters | LBP7680C/LBP7660C |  |  |
[Location] (SYS_LOC) | Up to 32 characters | (Blank) |  |  |
[Permit End-User's Job Operation] (USER_JOB_CONT) | ON, OFF | OFF |  |  |
Support Link
[URL] (LINK_URL1) | Up to 128 alphanumeric characters | http://www.canon.com |  |  |

#### TCP/IP (IP v. 4) Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use IPv4] (IPV4_USE) | ON, OFF | ON |  |  |
[DHCP] (DHCP_ENB) | ON, OFF | OFF |  |  |
[RARP] (RARP_ENB) | ON, OFF | OFF |  |  |
[BOOTP] (BOOTP_ENB) | ON, OFF | OFF |  |  |
[IP Address] (INT_ADDR) | IP address | 0.0.0.0 |  |  |
[Subnet Mask] (NET_MASK) | IP address | 0.0.0.0 |  |  |
[Gateway Address] (DEF_GW) | IP address | 0.0.0.0 |  |  |
[Primary DNS Server Address] (DNS_PADDR) | IP address | 0.0.0.0 |  |  |
[Secondary DNS Server Address] (DNS_SADDR) | IP address | 0.0.0.0 |  |  |
[Host Name] (HOST_NAME) | Up to 47 characters | "Canon" + "Last 6 digits of the MAC address" |  |  |
[Domain Name] (DOMAIN_NAME) | Up to 47 characters | (Blank) |  |  |
[DNS Dynamic Update] (DDNS_ENB) | ON, OFF | OFF |  |  |
[WINS Resolution] (WINS_ENB) | ON, OFF | OFF |  |  |
[WINS Server Address] (WINS_SERVER) | IP address | 0.0.0.0 |  |  |
[Scope ID] (WINS_SCOPEID) | Up to 63 characters | (Blank) |  |  |
[SMB Server Name] (SMB_SERVER) | Up to 15 alphanumeric characters | (Blank) |  |  |
[SMB Workgroup Name] (SMB_WG) | Up to 15 alphanumeric characters | (Blank) |  |  |
[Use ARP/PING] (ARP_PING_ENB) | ON, OFF | ON |  |  |
[Use FTP Print] (FTP_PRINT_ENB) | ON, OFF | OFF |  |  |
[FTP Print User Name] (FTP_PRINT_USER) | Up to 24 characters | (Blank) |  |  |
[Password] (FTP_PRINT_PWD) | Up to 24 characters | (Blank) |  |  |
[FTP Settings] | ON, OFF | OFF |  |  |
[Use LPD Printing] (LPD_ENB) | ON, OFF | ON |  |  |
[Print LPD Banner Page] (LPD_BANN) | ON, OFF | OFF |  |  |
[Use RAW Printing] (RAW_ENB) | ON, OFF | ON |  |  |
[Use Bidirectional Communication] (RAW_BIDIR_ENB) | ON, OFF | OFF |  |  |
[Use IPP Print] (IPP_ENB) | ON, OFF | OFF |  |  |
[SSL] | ON, OFF (Fixed at OFF when a key is not registered.) | OFF |  |  |
[IPP Authentication] (IPP_AUTH_ENB) | ON, OFF | ON |  |  |
[User Name] (IPP_AUTH_ACCUNT1) | Up to 24 characters (Must be entered when using IPP Authentication) | (Blank) |  |  |
[Password] (IPP_AUTH_PASSWD1) | Up to 24 characters (Must be entered when using IPP Authentication) | (Blank) |  |  |
[Use WSD Printing] (WSD_ENB) | ON, OFF | OFF |  |  |
[Use WSD Browsing] (WSD_BROWSING) | ON, OFF | OFF |  |  |
[Use Multicast Discovery] (WSD_MULTICAST_DISCOVERY) | ON, OFF | OFF |  |  |
[Use HTTP] (HTTP_ENB) | ON, OFF | ON |  |  |
[Use Proxy] | ON, OFF | OFF |  |  |
[HTTP Proxy Server Address] | Up to 128 alphanumeric characters | (Blank) |  |  |
[HTTP Proxy Server Port Number] | 0 to 99999 | 80 |  |  |
[Use Proxy Within Same Domain] | ON, OFF | OFF |  |  |
[Proxy Authentication] | ON, OFF | OFF |  |  |
[User Name] | Up to 24 alphanumeric characters | (Blank) |  |  |
[Password] | Up to 24 alphanumeric characters | (Blank) |  |  |
[Discovery Response] (DISCOVERY_ENB) | ON, OFF | ON |  |  |
[Scope Name] (DISCOVERY_SCOPE_NAME) | Scope name to be used for discovery using utility software such as NetSpot Device Installer. (Up to 32 characters *) | default |  |  |
[Use SNTP] (SNTP_ENB) | ON, OFF | OFF |  |  |
[NTP Server Name] (SNTP_ADDR) | IP address or host name | (Blank) |  |  |
[Polling Interval] (SNTP_INTERVAL) | Interval for synchronizing time (1 to 48 hours) | 24 |  |  |

* | You cannot use any of the following characters: "(", ")", ",", "!", "<", ">", "=", "~", ";", "+", "*", "\."

#### TCP/IP (IP v. 6) Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use IPv6] (IPV6_USE) | ON, OFF | OFF |  |  |
[Use Stateless Address] (IPV6_STATELESS_USE) | ON, OFF | ON |  |  |
[Use Manual Address] (IPV6_MANUAL_ADDR_USE) | ON, OFF | OFF |  |  |
[IP Address] (IPV6_MANUAL_ADDR_SET) | IP address | (Blank) |  |  |
[Prefix Length] (IPV6_MANUAL_ADDR_PREFIX) | 0 to 128 | 64 |  |  |
[Default Router Address] (IPV6_MANUAL_ROUTER_ADDR) | IP address | (Blank) |  |  |
[Use DHCPv6] (IPV6_DHCPV6_USE) | ON, OFF | OFF |  |  |
[Primary DNS Server Address] (IPV6_DNS_ADDRESS_PRI) | IP address | (Blank) |  |  |
[Secondary DNS Server Address] (IPV6_DNS_ADDRESS_SEC) | IP address | (Blank) |  |  |
[Use IPv4 Host/Domain Names] (IPV6_DNS_NAME_SAME_AS_IPV4) | ON, OFF | OFF |  |  |
[Host Name] (IPV6_DNS_HOST_NAME_V6) | Up to 47 characters | "Canon" + "Last 6 digits of the MAC address" |  |  |
[Domain Name] (IPV6_DNS_DOMAIN_NAME_V6) | Up to 47 characters | (Blank) |  |  |
[DNS Dynamic Update] (IPV6_DNS_DYNAMIC_SET) | ON, OFF | OFF |  |  |
[Register Manual Address] (IPV6_DNS_MANUAL) | ON, OFF | OFF |  |  |
[Register Stateful Address] (IPV6_DNS_STATEFUL) | ON, OFF | OFF |  |  |
[Register Stateless Address] (IPV6_DNS_STATELESS) | ON, OFF | OFF |  |  |

#### NetWare Network Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use NetWare] (NW_ENB) | ON, OFF | OFF |  |  |
[Frame Type] (NW_FRAME_TYPE) | Frame type used by NetWare | AutoSense ([Auto Detect]) |  |  |
[IPX External Network Number] | (Display only) |  |  |  |
[Node Number] | (Display only) |  |  |  |
[Print Service] (NW_PRINT_SERVICE) | Print service to be used | ndsPserver([NDS PServer]) |  |  |
Bindery PServer
[File Server Name] (NW_PSERVER_FILE_SERVER_ NAME) | Name of the NetWare file server to which the NetWare print server belongs (1 to 47 characters) | (Blank) |  |  |
[Print Server Name] (NW_PSERVER_PRINT_SERVER_NAME) | NetWare print server name to be used (1 to 47 characters) | (Blank) |  |  |
[Print Server Password] (NW_PSERVER_PASSWD) | Password for accessing the print server (0 to 20 characters) | (Blank) |  |  |
[Printer Number] (NW_PSERVER_PRINTER_NO) | Number for the printer connected to the NetWare print server (0 to 15) | 0 |  |  |
[Service Mode] (NW_PSERVER_SERVICE_MODE) | Service mode to be used psMode1: Only the currently loaded paper can be serviced. psMode2: Paper can be changed as needed. psMode3: The order of the jobs is rearranged to minimize the frequency of changing paper. psMode4: The order of the jobs in a queue is rearranged to minimize the frequency of changing paper. | psMode4 |  |  |
[Printer Form] (NW_PSERVER_PRINTER_FORM) | Paper Define Form (0 to 255) | 0 |  |  |
[Polling Interval] (NW_PSERVER_POLLING_INT) | Interval for checking the jobs (1 to 15 seconds) | 5 |  |  |
[Buffer Size] (NW_PSERVER_BUFFER_SIZE) | Data Buffer Size (1 to 20 KB) | 20 |  |  |
NDS PServer
[Tree Name](NW_NDSSERVER_TREE_NAME) | Name of the NDS tree to which the NetWare print server belongs (1 to 32 characters) | (Blank) |  |  |
[Context Name] (NW_NDSSERVER_CONTEXT_ NAME) | Name of the context to which the NetWare print server belongs (1 to 255 characters) | (Blank) |  |  |
[Print Server Name] (NW_NDSSERVER_PRINT_ SERVER_NAME) | NetWare print server name to be used (1 to 64 characters) | (Blank) |  |  |
[Print Server Password] (NW_NDSSERVER_PRINT_ SERVER_PASSWORD) | Password for accessing the print server (0 to 20 characters) | (Blank) |  |  |
[Printer Number] (NW_NDSSERVER_PRINTER_NO) | Number for the printer connected to the NetWare print server (0 to 254) | 0 |  |  |
[Service Mode] (NW_NDSSERVER_SERVICE_ MODE) | Service mode to be used psMode1: Only the currently loaded paper can be serviced. psMode2: Paper can be changed as needed. psMode3: The order of the jobs is rearranged to minimize the frequency of changing paper. psMode4: The order of the jobs in a queue is rearranged to minimize the frequency of changing paper. | psMode4 |  |  |
[Printer Form] (NW_NDSSERVER_PRINTER_FORM) | Paper Define Form (0 to 255) | 0 |  |  |
[Polling Interval] (NW_NDSSERVER_POLLING_INT) | Interval for checking the jobs (1 to 255 seconds) | 5 |  |  |
[Buffer Size] (NW_NDSSERVER_BUFFER_SIZE) | Data Buffer Size (3 to 20 KB) | 20 |  |  |
RPrinter
[File Server Name] (NW_RPRINTER_FILE_SERVER_ NAME) | Name of the NetWare file server to which the NetWare print server belongs (1 to 47 characters) | (Blank) |  |  |
[Print Server Name] (NW_RPRINTER_PRINT_SERVER_ NAME) | NetWare print server name to be used (1 to 47 characters) | (Blank) |  |  |
[Printer Number] (NW_RPRINTER_PRINTER_NO) | Number for the printer connected to the NetWare print server (0 to 15) | 0 |  |  |
NPrinter
[Tree Name](NW_NPRINTER_TREE_NAME) | Name of the NPrinter tree to which the NetWare print server belongs (1 to 32 characters) | (Blank) |  |  |
[Context Name] (NW_NPRINTER_CONTEXT_NAME) | Name of the context to which the NetWare print server belongs (1 to 256 characters) | (Blank) |  |  |
[Print Server Name] (NW_NPRINTER_PRINT_SERVER_ NAME) | NetWare print server name to be used (1 to 64 characters) | (Blank) |  |  |
[Printer Number](NW_NPRINTER_PRINTER_NO) | Number for the printer connected to the NetWare print server (0 to 254) | 0 |  |  |

#### AppleTalk Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use AppleTalk] (ATLK_ENB) | ON, OFF | OFF |  |  |
[Phase] | Fixed at [Phase 2] | [Phase 2] |  |  |
[Service Name] (APRINT_1) | Up to 32 characters *1 | LBP7680Cx/LBP7660Cdn |  |  |
[Zone] (ATK_ZONE) | Up to 32 characters *2 | * |  |  |
[Print Mode]*3 | [Open Both Spool and Direct], [Open Spool], [Open Direct] | [Open Both Spool and Direct] |  |  |

*1 | "=", "@", "*", ":", and "~" cannot be used.
*2 | "=", "@", ":", and "~" cannot be used.
*3 | Can be specified only when PS ROM or PS/Barcode ROM is installed.

#### SMB Settings (LBP7680Cx Only)

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use SMB Server](SMB_ENB) | ON, OFF | OFF |  |  |
[Server Name](SMB_SERVER) | Up to 15 characters * | (Blank) |  |  |
[Workgroup Name](SMB_WG) | Up to 15 characters * | (Blank) |  |  |
[Comments](SMB_COMMENT) | Up to 48 characters | (Blank) |  |  |
[Use LM Announce](SMB_LM_ENB) | ON, OFF | OFF |  |  |
[Use SMB Printing](SMB_PRINT_ENB) | ON, OFF | OFF |  |  |
[Printer Name](SMB_PRINTER) | Up to 13 characters * | (Blank) |  |  |

* | You cannot enter a space between characters.

#### SNMP Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use SNMPv1] (SNMP_V1_ENB) | ON, OFF | ON |  |  |
[Use Community Name 1] (SNMP_COMMUNITY1_ENB) | ON, OFF | ON |  |  |
[Community Name 1] (SNMP_COMMUNITY1_NAME) | Up to 32 characters | public |  |  |
[MIB Access Permission] (SNMP_COMMUNITY1_ACCESS) | RW, RO ([Read/Write], [Read Only]) | RO ([Read Only]) |  |  |
[Use Community Name 2] (SNMP_COMMUNITY2_ENB) | ON, OFF | OFF |  |  |
[Community Name 2] (SNMP_COMMUNITY2_NAME) | Up to 32 characters | public2 |  |  |
[MIB Access Permission] (SNMP_COMMUNITY2_ACCESS) | RW, RO ([Read/Write], [Read Only]) | RO ([Read Only]) |  |  |
[Use SNMPv3] (SNMP_V3_ENB) | ON, OFF | OFF |  |  |
[Obtain Printer Management Information from Host] (SNMP_GET_PRT_MNG_INFO) | ON, OFF | OFF |  |  |
[Reject SNMP Packets While in Sleep Mode] | ON, OFF | OFF |  |  |

#### User Settings (SNMPv3)

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[User Name] | Up to 32 alphanumeric characters | initial |  |  |
[MIB Access Permission] | [Read/Write], [Read Only] | [Read/Write] |  |  |
[Security Settings] | [Authentication Yes/Encryption Yes], [Authentication Yes/Encryption No], [Authentication No/Encryption No] | [Authentication Yes/Encryption Yes] |  |  |
[Authentication Algorithm] | [MD5], [SHA1] | [MD5] |  |  |
[Authentication Password] * | 6 to 16 alphanumeric characters | initial |  |  |
[Encryption Algorithm] | [DES], [AES] | [DES] |  |  |
[Encryption Password] * | 6 to 16 alphanumeric characters | initial |  |  |

* | Can be specified only when the printer is in the state of SSL encrypted communication. (If the printer is not in the state of encrypted communication, specify the setting using the printer's control panel.)

#### Context Settings (SNMPv3)

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Context Name 1] - [Context Name 5] | Up to 32 alphanumeric characters | (Blank) |  |  |

#### Spooler Settings (LBP7680Cx Only)

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Use Spooler](SPOOL_ENB) | ON, OFF | OFF |  |  |

#### Startup Time Setting

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Startup Time] (STRT_DELAY_TIME) | Waiting time from when you turn the printer ON to when the printer starts obtaining the address (0 to 300 seconds) | 0 |  |  |

#### Ethernet Driver Setting

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Auto Detect] | ON, OFF | ON |  |  |
[Communication Mode] | [Half Duplex], [Full Duplex] | [Half Duplex] |  |  |
[Ethernet Type] | [10 Base-T], [100 Base-TX], [1000 Base-T] | [10 Base-T] |  |  |

#### E-Mail Print Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[POP3 Server Name](EMAIL_POP_ADDR) | Up to 48 characters | (Blank) |  |  |
[POP3 User Name](EMAIL_POP_ACCOUNT) | Up to 32 characters | (Blank) |  |  |
[Password](EMAIL_POP_PASSWD) | Up to 32 characters | (Blank) |  |  |
[POP3 RX Interval](EMAIL_POP_INTERVAL) | 0 to 90 minutes | 0* |  |  |
[POP3 RX](EMAIL_PRINT_ENB) | ON, OFF | OFF |  |  |
[POP3 Server Port Number](EMAIL_POP_PORTNO) | 0 to 65535 | 110 |  |  |
[SMTP RX] | ON, OFF | OFF |  |  |
[SMTP Server Port Number] | 0 to 65535 | 25 |  |  |

* | When [0] is set, auto e-mail reception to the server is not performed.

#### Remote UI Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[Remote UI](RUI_ENB)* | Turing ON or OFF the Remote UI | ON |  |  |
[Use SSL] | ON, OFF | OFF |  |  |

* | Can be specified only by FTP Client or the printer's control panel

#### Permitted Receiving MAC Address Settings

: Can be specified: Cannot be specified

Option | Contents | Default | Settings Using NetSpot Device Installer | Settings Using FTP Client | Settings Using the Control Panel
[MAC Address Filter] | ON, OFF | OFF |  |  |
[MAC Address] | (Display only) |  |  |  |

## Software That Can Be Used for the Network Settings

You can perform the network settings for this printer using the following software.

: | Specifiable
: | Not specifiable
: | Can perform a part of the settings

Setting Type | Web Browser (Remote UI) | FTP Client | NetSpot Device Installer | ARP/PING Command | Control Panel of the Printer
Configuring the Ethernet Driver "Changing the Network Transmission Speed or Transfer Mode" |  |  |  |  |
Setting the Spooling Function (LBP7680Cx only) "Setting the Spooling Function (LBP7680Cx Only)" |  |  |  |  |
Configuring the Communication Environment "Specifying the Setting for Startup Waiting Time" |  |  |  |  |
Setting the IP Address of the Printer "Setting the IP Address (IP v. 4)" |  |  |  |  |
Setting the TCP/IP Protocol "Configuring the Protocol Settings" |  |  |  |  |
Setting IP v. 6 "Setting IP v. 6" |  |  |  |  |
Preparing the NetWare Protocol Settings "Configuring NetWare" |  |  |  |  |
Setting the NetWare Protocol "Configuring the Protocol Settings" |  |  |  |  |
Setting the AppleTalk Protocol "Network Settings for the Printer (AppleTalk)" |  |  |  |  |
Changing the Device Name or Administrator Information "Specifying the Device Name or Administrator Information" |  |  |  |  |
Changing the Administrator Password "Setting the Administrator Password" |  |  |  |  |
Specifying the Job Operation Permission for End-users "Specifying the Job Operation Permission for End-Users" |  |  |  |  |
Restricting the Job Requests by Certain Devices "Restricting the Users Who Can Print or Perform the Printer Settings" |  |  |  |  |
Restricting the Job Requests by Certain Devices "Restricting the Users Who Can Print or Perform the Printer Settings" |  |  |  |  |
Keylock Settings "Locking the Keys on the Control Panel (Key Lock Function)" |  |  |  |  |
Changing E-Mail Print Settings "Receiving E-mail Data on the Mail Server and Printing (E-mail Print)" |  |  |  |  |

0258-06L