# 2-sided Printing

You can print a document on both sides of the paper.

Paper Type | Paper Size
Plain paper (60 to 90 g/m²) Heavy paper (91 to 120 g/m²) | Standard size: A4, Legal, Letter Custom size: 127.0 to 215.9 mm wide and 279.4 to 355.6 mm long

Before performing 2-sided printing, see "Attention (1-sided Printing and 2-sided Printing)."

IMPORTANT
###### Precautions when performing 2-sided printing Do not touch the paper during 2-sided printing until it is output completely. The paper is first output partially after the front side is printed, and then it is fed again to be printed on the reverse side. Be sure to close the output selection cover before performing 2-sided printing. "Paper Loading and Output" ###### Printing on the reverse side of paper that was previously printed (Performing 2-sided printing manually) Using the multi-purpose tray, this printer enables you to perform 2-sided printing manually by inserting the reverse side of the paper* that was previously printed. When printing on the reverse side of paper that was previously printed, flatten the curl and load one sheet of paper at a time in the multi-purpose tray.
* | You can use only paper printed by this printer. Also, you cannot print on the printed side again.

1.
Select [Print] from the [File] menu of the application.
2.
Select your printer from [Printer] → [Finishing] → [2-sided Printing] from [Print Style].
3.
Select the binding edge from [Binding Location].
The output image is displayed in the preview area.
4.
If you want to set the gutter width, click [Gutter].
If you do not set the gutter width, skip to step 6.
5.
Specify the gutter width → click [OK].
6.
Click [Print].

NOTE
The screen may vary according to the operating system, as well as the type and version of the printer driver.

0258-05W