# Selecting the Receive Mode

Select the receive mode that suits your intended use beforehand (Deciding Which Fax Receive Mode to Use).
1
Tap <Next>.
The screen shown here is displayed after the unit name has been registered (Registering the Fax Number and Unit Name).
2
Select the receive mode that suits your intended use.
Tap <Yes> or <No> to select the receive mode.
If you have subscribed to a Distinctive Ring Pattern Detection (DRPD) service provided by your telephone company, <DRPD> is also available for the receiving mode. Receiving Faxes
To set the receive mode to <Auto>
To set the receive mode to <Fax/Tel Auto Switch>
To set the receive mode to <Answering Machine>
To set the receive mode to <Manual>
3
Tap <Apply>.
If the machine is set to <Answering Machine>, tap <Next>.
»
Continue to Connecting the Telephone Line
LINKS
Receiving Faxes
0Y01-02C