# Setting Up Connection by Selecting a Wireless Router

You can search the wireless routers (or access points) available for connection and select one from the display of the machine. For the network key, enter a WEP key or PSK. Before selecting a wireless router, check and write down the required setup information, including the SSID and network key (Checking the SSID and Network Key).

##### Security settings If the wireless connection is set up by selecting a wireless router, the WEP authentication method is set to <Open System> or the WPA/WPA2 encryption method is set to <Auto> (AES-CCMP or TKIP). If you want to select <Shared Key> for WEP authentication or <AES-CCMP> for WPA/WPA2 encryption, you need to set up the connection using the manual entry method (Setting Up Connection by Specifying Detailed Settings).

1
Tap <Menu> in the Home screen.
2
Tap <Network Settings>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
3
Tap <Wireless LAN Settings>.
If the <Do you want to enable the wireless LAN?> message is displayed, tap <Yes>.
4
Read the message that is displayed, and tap <OK>.
5
Tap <SSID Settings>.
6
Tap <Select Access Point>.
The machine starts searching for available wireless routers.
If <Cannot find the access point.> is displayed, see When an Error Message Appears.
7
Select a wireless LAN router.
Tap the router whose SSID matches the one that you have written down.
To view details of security settings
Tap <Details> and select the wireless LAN router. To return to the original screen, tap <Close> twice, and then press .
If your wireless router is not found
Check whether the machine is properly installed and ready to connect to the network. Installation/Settings Problems
8
Enter the network key that you have written down.
Enter the network key using the numeric keys, and tap <Apply>.
On how to enter text, see Entering Text.

| WEP |  | WPA-PSK or WPA2-PSK |  |  |  |  |  |  |  |  |

9
Tap <Yes>.
If an error message is displayed during setup
Tap <Close>, check whether the network key is correct, and return to step 5.
10
Check that the Wi-Fi indicator is blinking on the operation panel.
The Wi-Fi indicator blinks when a wireless router is detected.
When the setup is completed, the screen below is displayed, and approximately 2 seconds later, the Wi-Fi indicator lights up. Wait approximately 2 minutes (until the automatic settings of IP address and other items are complete).
Signal strength
When more than one wireless router is available for connection, the machine connects to the device with the strongest signal. Signal strength is measured using RSSI (Received Signal Strength Indication).
You can set the IP address manually. Setting IP Addresses

##### Reducing power consumption You can set the machine to enter <Power Save Mode> based on signals emitted from the wireless router. Power Save Mode ##### If the IP address of the machine has changed In a DHCP environment, the IP address of the machine may be changed automatically. If this happens, the connection is maintained as long as the machine and the computer belong to the same subnet.

LINKS
Connecting to a Wireless LAN
0Y01-079