# Machine Specifications

Type | Personal Desktop
Power Supply | 120 to 127 V, 60 Hz (Power requirements differ depending on the country in which you purchased the product.)
Power Consumption | Maximum 1,450 W or less During standby mode Approx. 11.2 W (USB connection) Approx. 11.3 W (wired LAN connection) Approx. 11.8 W (wireless LAN connection) During sleep mode Approx. 0.7 W (USB connection) Approx. 0.8 W (wired LAN connection) Approx. 1.4 W (wireless LAN connection) When the power switch is turned OFF 0.1 W or less
Warm-up Time*1 (From power ON until machine enters standby) | 16 seconds or less
Weight*2 | Approx. 53.6 lb (24.3 kg)
Dimensions (W x L x H) | In the normal state 17 7/8" x 18 3/4" x 19 7/8" (453 x 477 x 503 mm) When the two optional paper feeders are installed 17 7/8" x 18 3/4" x 30 3/4" (453 x 477 x 780 mm) When the optional handset is installed 20 7/8" x 18 3/4" x 19 7/8" (530 x 477 x 503 mm)
Environmental Conditions | Temperature: 50 to 86°F (10 to 30°C) Humidity: 20% to 80% RH (no condensation)
Host Interface | 1000BASE-T 100BASE-TX 10BASE-T Hi-Speed USB USB IEEE 802.11b/g/n (Infrastructure mode)
Noise (measured in accordance with ISO 7779, declared noise emission in accordance with ISO 9296) | LwAd (Declared A-weighted sound power level (1 B = 10 dB)) During standby mode: Inaudible*3 During printing: 6.9 B or less (1-sided) During printing: 6.7 B or less (2-sided) LpAm (Declared A-weighted emission sound pressure level (Bystander position)) During standby mode: Inaudible*3 During printing: Approx. 54 dB (1-sided) During printing: Approx. 52 dB (2-sided)
Gradation | 256 gradations
Acceptable Documents | Supported Document Types
Acceptable Paper Stock | Paper
Printable Range | Printable Area
Scan Range | Scan Area
*1 Warm-up time may vary depending on the use conditions and environment of the machine. *2 The value indicates the mass of the main unit including toner cartridges. *3 Indicates that the sound pressure level of each bystander position is below the ISO 7779 absolute criteria for the background noise level.

0Y01-0F1