# Configuring FTP PASV mode

|  | PASV is an FTP communication mode used for file transfer. To connect to an FTP server through a firewall, you must use PASV mode. First check that the PASV mode is set on the FTP server.

Whether PASV mode is used for FTP depends on your network environment and the settings on the FTP server to which data is being sent. For more information, contact your Network Administrator.

1
Start the Remote UI and log on in System Manager Mode. Starting Remote UI
2
Click [Settings/Registration].
3
Click [Network Settings] [TCP/IP Settings].
4
Click [Edit] in [FTP PASV Mode Settings].
5
Select the [Use FTP PASV Mode] check box and click [OK].
[Use FTP PASV Mode]
Select the check box to use PASV mode. If you are not using PASV mode, leave the check box clear.
6
Restart the machine.
Turn OFF the machine, wait for at least 10 seconds, and turn it back ON.
0Y01-083