# Receiving Faxes

This section describes the methods for receiving faxes and how to set up the machine to receive faxes. You need to complete some procedures for using fax functions before specifying the receiving settings. Configuring Initial Settings for Fax Functions

The machine can print received fax documents on A4 or Letter size paper. If received fax documents are printed on other paper sizes, a portion of the page may not be printed or a page may be printed on two separate sheets of paper.

### Methods for Receiving Faxes

The machine provides the following receiving methods. Select the method that best suits your needs and then set it up by following the procedures in Setting Up the Machine to Receive Faxes.

<Auto> | Dedicated to receiving faxes The machine receives faxes automatically. Even if someone makes a call to you, you cannot talk to the caller.
<Fax/Tel Auto Switch> | When the call is a fax The machine receives the fax automatically. When the call is a telephone call An incoming call rings. Pick up the handset to answer the call. You need to connect your telephone or the optional handset to the machine beforehand.
<Manual> | When the call is a fax An incoming call rings. Pick up the handset. If you hear a beep, tap <Fax> <Start Receiving> to receive faxes. When the call is a telephone call An incoming call rings. Pick up the handset and start your conversation. You need to connect your telephone or the optional handset to the machine beforehand. You can set the machine to automatically receive faxes when an incoming call rings within a specified timeframe. Switch to Auto RX
<Answering Machine> | When the call is a fax After an incoming call rings, the machine receives the fax automatically. When the call is a telephone call The answering machine activates, enabling the caller to leave a message. If you pick up the handset before the answering machine starts recording a message, you can talk with the caller. You need to connect your answering machine to the machine beforehand. Set the answering machine to answer after a few rings. We recommend that you add approximately 4 seconds of silence at the beginning of the message or set the maximum recording time to 20 seconds.
<DRPD> | If you have subscribed to a Distinctive Ring Pattern Detection (DRPD) service provided by your telephone company, this receiving mode is available. This service assigns two or more telephone numbers with distinctive ring patterns to a single telephone line. You can use one of these numbers for faxes and one for telephone calls. When the machine receives a call, it automatically recognizes the ring pattern and your telephone rings differently depending on whether the call is a fax or telephone call. If the ring pattern is for a fax, the machine automatically receives the fax. For more information about this service, contact your telephone company. You need to connect your telephone or the optional handset to the machine beforehand.

Depending on the type of telephone connected to it, the machine may not be able to send or receive faxes properly. If you are connecting an external telephone with fax functions, set the telephone to not receive faxes automatically. If you pick up the telephone handset and hear a beep, the call is a fax. You can receive the fax just by using the telephone to enter a specific ID number. Using a Telephone to Receive Faxes (Remote Reception)

### Setting Up the Machine to Receive Faxes

1
Press and tap <Fax>.
When the logon screen appears, use the numeric keys to enter the user name and password. Then select the authentication server and press . Logging on to Authorized Send
2
Tap <RX Mode>.
3
Select the receiving method.

###### When selecting <Fax/Tel (Auto Switch)>

Specify the following three settings as necessary. When the setting is complete, tap <Apply>.

#### <Ring Start Time>

Enables you to specify the duration during which the machine determines whether an incoming call is a fax or a telephone call. (Setting values: 5 to 30 seconds; default setting: 6 seconds)

#### <Incoming Ring Time>

Enables you to specify the duration during which an incoming call rings for a telephone call. (Setting values: 15 to 300 seconds; default setting: 15 seconds)

#### <After Ring>

Enables you to specify how the machine operates if you do not pick up the handset while an incoming call is ringing. Select <End> to disconnect the call or <Receive> to receive an incoming fax. (Default setting: <Receive>)

###### When selecting <DRPD>

Select the ring pattern that your telephone company assigned to your fax number.

If you want to print received documents on both sides of paper: Print on Both Sides If you want to print information, such as reception date and time, at the bottom of received documents: RX Page Footer If you want to continue printing even when the toner cartridge is low: Continue Printing When Amount in Cartridge Is Low

### Using a Telephone to Receive Faxes (Remote Reception)

When you pick up the telephone and get a fax signal, you do not need to go to the machine to receive the fax. Just enter a specific ID number (default setting: 25) with the telephone, and you can start receiving the fax.

When the telephone is not directly connected with the machine, the remote reception function is not available.

1
When an incoming call rings, pick up the telephone handset.
2
If you hear a beep, enter the ID number for Remote Reception with the telephone.
The ID number is set to "25" by default. You can change this number as necessary. Remote RX
3
Hang up the handset.
LINKS
Sending and Receiving Faxes According to Your Purposes
Checking Status and Log for Sent and Received Documents
0Y01-034