# Adjusting the Volume

The machine produces sounds in a variety of situations, such as when fax sending is complete or when a paper jam or error occurs. You can set the volume of each of these sounds individually.

### Adjusting <Fax Volume>

1
Press the () key.
2
To change <Fax Volume>, tap /, and tap <Apply>.
You can also adjust the volume by flicking the slider.
Tap and move the cursor all the way to the left to mute the sound.

### Adjusting <Other Volume>

1
Press () key.
2
Tap <Other Volume>.
3
Select a setting.

Setting | Description | Procedure
<Ring Tone> | Sound produced when an incoming fax is received | Go to step 4.
<TX Done Tone> | Sound produced when fax sending is complete
<RX Done Tone> | Sound produced when fax receiving is complete
<Scanning Done Tone> | Sound produced when fax document scanning is complete
<Entry Tone> | Confirmation sound each time a key on the operation panel or button on the display is pressed | Select <On> (produce a tone) or <Off> (not produce a tone).
<Invalid Entry Tone> | Sound produced when an invalid key operation is performed, such as when you enter a number outside the valid setting range
<Restock Supplies Tone> | Sound produced when a toner cartridge is almost empty
<Warning Tone> | Sound produced when a paper jam or other error occurs
<Job Done Tone> | Sound produced when an operation such as copying or scanning is complete
<Energy Saver Alert> | Sound produced when the machine enters or exits sleep mode
<Original in Feeder Detection Tone> | Sound produced when an original is loaded in the feeder

4
Use / to set volume, tap <Apply>.
Tap and move the cursor all the way to the left to mute the sound.

###### For sound to be produced only when an error has occurred

Tap <Only When Err.> <On> <Apply>.
0Y01-01C