# Front Side

#### Feeder

Automatically feeds documents into the machine for scanning. When two or more sheets are loaded in the feeder, documents can be scanned continuously. Placing Documents

#### Ventilation slots

Air from inside the machine is vented out to cool down the inside of the machine. Note that placing objects in front of the ventilation slots prevents ventilation. Installation

#### Lift handles

Hold the lift handles when carrying the machine. Relocating the Machine

#### Operation panel

The operation panel consists of keys such as the numeric keys and [Start] key, a display, and status indicators. You can perform all the operations and specify settings from the operation panel. Operation Panel Display

#### USB port (for USB device connection)

Use this port to connect a USB memory device or USB keyboard. Connecting a USB memory device allows you to print data from the memory device or save scanned documents to the memory device. Printing from USB Memory (Memory Media Print) Scanning Documents Directly to USB Memory

#### Front cover

Open the front cover when replacing the toner cartridge or clearing paper jams. How to Replace Toner Cartridges Clearing Jams

#### Paper drawer

Load the type of paper you frequently use into the paper drawer. Loading Paper in the Paper Drawer

#### Multi-purpose tray

Load the paper into the multi-purpose tray when you want to temporarily use a type of paper different from that which is loaded in the paper drawer. Loading Paper in the Multi-Purpose Tray

#### Scanning area

Documents loaded in the feeder are automatically fed to the scanning area for scanning.

#### Output tray

Printed paper is output to the output tray.

#### Paper stopper

Open the paper stopper to prevent paper in the output tray from falling.

#### Platen glass

Place documents to scan on the platen glass. Also, use the platen glass to place thick or bound documents such as books when they cannot be loaded in the feeder. Placing Documents

#### Speaker

Emits sounds produced by the machine, such as fax tones and warning tones.

#### Power switch

Turns the power ON or OFF. To restart the machine, turn OFF the machine, wait for at least 10 seconds, and turn it back ON.
0Y01-008