# Receiving I-Faxes

### When an I-Fax Arrives

When an I-Fax arrives, the [Processing/Data] indicator on the operation panel blinks. After the I-Fax is completely received, the document is printed out automatically and the indicator goes out.

To cancel reception, press <RX Job> <Job Status> Select the document on the <RX Job Status> screen <Delete> <Yes>

### Receiving I-Faxes Manually

If you want to connect to the server before receiving I-Faxes automatically, or if you want to configure the machine so that it does not receive I-Faxes automatically, use the method below to receive I-Faxes manually.
<RX Job> <Check I-Fax RX>
Connect to the server. If there is a document on the server, printing begins.

### Printout Paper

Regardless of the received document size, incoming I-Faxes are printed at the size specified in <RX Print Size>. RX Print Size

If paper of the size specified in <RX Print Size> is not loaded in the paper drawer, the <No Paper> error message is displayed. When an Error Message Appears

If you want to print received documents on both sides of paper: Print on Both Sides If you want to continue printing even when toner is running low: Continue Printing When Amount in Cartridge Is Low

LINKS
Checking Status and Log for Sent and Received Documents
0Y01-040