# Relocating the Machine

The machine is heavy. Make sure to follow the procedures below when moving the machine to avoid injury, and also make sure to read the safety precautions before you begin. Important Safety Instructions
1
Turn OFF the machine and computer.
When you turn OFF the machine, data that is waiting to be printed is deleted. Fax documents that were received by using the Memory Reception function, faxes that are waiting to be sent, and reports that are automatically printed after sending and receiving faxes are not deleted.
2
Disconnect the cables and cord from the machine in numerical order as in the illustration below.
Whether the cables with "*" are connected depends on your environment.
When the optional handset is connected, remove it from the rack.

Power plug Power cord USB keyboard* USB cable* LAN cable* Handset cable* External telephone cable* Telephone cable* |

3
When transporting the machine across a long distance, remove the toner cartridge. How to Replace Toner Cartridges
4
Pull out the paper drawer.
Make sure to hold the paper drawer with both hands, and pull it out gently. Otherwise, you may damage the paper drawer by dropping it, if it slides out too easily.
5
Close all the open covers, and move the machine to a new location.
The machine is heavy (Machine Specifications). Make sure to move the machine with two or more people.
Hold the lift handles, then lift up the machine. If you have attached the optional paper feeder, leave the optional paper feeder on the floor and move it after moving the main unit of the machine.
6
Carefully place the machine at the new installation site.
For information about how to install the machine after relocating it, see "Getting Started." Manuals Included with the Machine
0Y01-0CR