# Configuring Ethernet Settings

|  | Ethernet is a standard for communicating data in a local area network (LAN). You can set the communication mode (half-duplex/full-duplex) and the Ethernet type (10BASE-T/100BASE-TX/1000BASE-T). In general, the machine can be used without changing the defaults (Ethernet Driver Settings), but you can change these settings to suit your network environment.

1
Tap <Menu> in the Home screen.
2
Tap <Network Settings>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
3
Select <Ethernet Driver Settings> <Auto Detect>.
4
Select whether to configure Ethernet settings automatically or manually.

###### Configuring Ethernet settings automatically

Tap <On>. The machine detects and automatically sets the communication mode and the Ethernet type that can be used.

###### Configuring Ethernet settings manually

1 | Tap <Off>.
2 | Select the communication mode. Tap <Communication Mode> tap <Half Duplex> or <Full Duplex>. <Half Duplex> Alternately sends and receives communication data. Select when the machine is connected to a networking device using half duplex. <Full Duplex> Simultaneously sends and receives communication data. Use this setting for most environments.
3 | Select the Ethernet type. Tap <Ethernet Type> select the Ethernet type. When <Communication Mode> is set to <Half Duplex>, you cannot select <1000BASE-T>.
4 | Tap <Apply>.

5
Restart the machine.
Turn OFF the machine, wait for at least 10 seconds, and turn it back ON.
LINKS
Changing the Maximum Transmission Unit
Setting a Wait Time for Connecting to a Network
0Y01-085