# Fax Specifications

Line Used | Public Switched Telephone Network (PSTN) *1
Communication Mode | Super G3, G3
Compression Method | MH, MR, MMR, JBIG
Modem Speed | Super G3: 33.6 Kbps, G3: 14.4 Kbps Automatic Fallback
Transmission Speed | Approx. 3 seconds per page *2 (ECM-JBIG, transmitting from the memory at 33.6 Kbps)
Sending from Memory/Receiving in Memory | Maximum approx. 512 pages *2 (Total pages of transmission/reception) (Maximum number of fax jobs that can be sent from the memory: 30 jobs/Maximum number of fax jobs that can be received into the memory: 90 jobs)
Fax Resolution | Normal: 200 x 100 dpi Fine: 200 x 200 dpi Photo: 200 x 200 dpi Superfine: 200 x 400 dpi Ultrafine: 400 x 400 dpi
Dialing | Favorites (19 destinations) Coded dialing (281 destinations) Group dialing (299 destinations) Address Book dialing Regular dialing (with numeric keys) Automatic redialing Manual redialing Sequential broadcast (310 destinations)
Receiving | Automatic reception Manual reception Remote reception by telephone (Default ID: 25)
Reports | TX Result Report Communication Management Report (By default, auto output every 40 destinations) RX Result Report
Telephone Type | Handset (optional) External telephone External telephone with the built-in answer function Data modem
*1 Depending on your locale or your telephone connection, you may be unable to perform data communication. In this case, contact your local authorized Canon dealer or the Canon help line. *2 Based on ITU-T (ITU Telecommunication Standardization Sector) Standard Chart No. 1, JBIG standard mode.

0Y01-0F7