# Prohibiting Sequential Broadcasting

Sequential broadcasting is a feature that sends faxes to multiple recipients in succession. This feature can be disabled if preferred.
1
Tap <Menu> in the Home screen.
2
Tap <Fax Settings>.
3
Select <Restrict TX Function> <Restrict Sequential Broadcast>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
4
Select <Confirm Sequential Broadcast> or <Reject Sequential Broadcast>.
<Off>
Enables sequential broadcasting.
<Confirm Sequential Broadcast>
Displays the confirmation screen when sending a fax via sequential broadcasting.
<Reject Sequential Broadcast>
Disables sequential broadcasting.
LINKS
Limiting Available Destinations
Disabling Use of Previously Used Destinations
Sending Faxes to Multiple Destinations Simultaneously (Sequential Broadcast)
0Y01-09C