# Setting IPv4 Address

|  | The machine's IPv4 address can be either assigned automatically by a dynamic IP addressing protocol, such as DHCP, or entered manually. When connecting the machine to a wired LAN, make sure that the connectors of the LAN cable are firmly inserted into the ports (Connecting to a Wired LAN). You can test the network connection if necessary.

Setting IPv4 Address
Testing the Network Connection

## Setting IPv4 Address

1
Tap <Menu> in the Home screen.
2
Tap <Network Settings>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
3
Select <TCP/IP Settings> <IPv4 Settings> <IP Address Settings>.
4
Configure IP address settings.
<Auto Acquire>
Select to automatically assign an IP address via DHCP protocol. When <Auto Acquire: On> is displayed, automatic addressing is enabled.
<Manually Acquire>
Select to configure the IP address settings by manually entering an IP address. In order to select this option, <Auto Acquire> must be set to <Off>.
<Check Settings>
Select when you want to view the current IP address settings.

###### Automatically assigning an IP address

1 | Select <Auto Acquire> <Select Protocol>.
2 | Tap <DHCP>. If you do not want to use DHCP to assign an IP address Tap <Off>. If you select <DHCP> when this service is unavailable, the machine will waste time and communications resources searching the network for this service.
3 | Check that <Auto IP> is set to <On>. If <Off> is selected, change the setting to <On>.
4 | Tap <Apply>.

IP addresses assigned via DHCP override the address obtained via Auto IP.

###### Manually entering an IP address

1 | Check that <Auto Acquire> is set to <Off>. If <On> is displayed, tap <Auto Acquire>, and set both <Select Protocol> and <Auto IP> to <Off>.
2 | Tap <Manually Acquire>.
3 | Specify the IP address, subnet mask, and gateway address (or default gateway). Specify the settings in the following order: <IP Address> <Subnet Mask> <Gateway Address>. Enter each setting using the numeric keys, and tap <Apply>.

5
Restart the machine.
Turn OFF the machine, wait for at least 10 seconds, and turn it back ON.

##### Checking whether the settings are correct Make sure that the Remote UI screen can be displayed with your computer (Starting Remote UI). If a computer is not available, you can check the connection by using the operation panel (Testing the Network Connection). ##### If you changed the IP address after installing the printer driver If you are using an MFNP port, and the machine and the computer are on the same subnet, then the connection will be maintained. You do not need to add a new port. If you are using a standard TCP/IP port, then you need to add a new port. Configuring Printer Ports * If you are not sure which type of port you are using, see Checking the Printer Port.

## Testing the Network Connection

1
Tap <Menu> in the Home screen.
2
Tap <Network Settings>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
3
Select <TCP/IP Settings> <IPv4 Settings> <PING Command>.
4
Enter the IPv4 address of another device on the network, and tap <Apply>.
If a proper connection has been established, the following screen is displayed.
LINKS
Setting IPv6 Addresses
Viewing Network Settings
Configuring WINS
0Y01-07F