# Paper Creases or Curls

## Paper Creases

#### Is paper loaded correctly?

If paper is not loaded below the load limit line or the load limit guide or is loaded obliquely, it may crease.
Loading Paper

#### Are you using paper that has absorbed moisture?

Replace with appropriate paper.
Loading Paper
Change the setting for <Paper Wrinkle Correction>. The improvement effect is stronger with <Mode 2> than with <Mode 1>. First try the adjustment with <Mode 1>.
Paper Wrinkle Correction
Printing speed becomes slower when you select stronger improvement.

#### Are you using appropriate paper?

Check usable paper, and replace with appropriate paper.
Paper
Loading Paper

## Paper Curls

#### Are you using paper that has absorbed moisture?

Replace with appropriate paper.
Loading Paper
When the current setting of <Paper Type> is <Plain>, change it to <Plain L>.
Specifying Paper Size and Type
Change the setting for <Paper Curl Correction>. The improvement effect is stronger with <Mode 2> than with <Mode 1>. First try the adjustment with <Mode 1>.
Paper Curl Correction
If the improvement effect becomes stronger, it may take some time to start printing.
Printing speed may become slower depending on the paper size.

#### Are you using appropriate paper?

Check usable paper, and replace with appropriate paper. Also, specify the paper size and type settings properly.
Paper
Loading Paper
Specifying Paper Size and Type

#### Are you outputting printed paper to the output tray?

If envelopes or other type paper are curled, output printed paper to the sub-output tray on the back side of the machine.
0Y01-0C6