# Checking Destinations before Sending Documents

By entering the fax number twice, you can reduce the risk of faxing to the wrong number due to input mistakes. Use features described in this section if you send confidential documents.
Displaying the Screen for Confirming the Fax Number
Displaying Destinations in Address Book

## Displaying the Screen for Confirming the Fax Number

You can set the machine to ask users to enter the fax number twice when it is entered by using the numeric keys. This way, you can reduce the risk of faxing to the wrong number due to input mistakes.
1
Tap <Menu> in the Home screen.
2
Tap <Fax Settings>.
3
Select <TX Function Settings> <Confirm Entered Fax Number>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
4
Tap <On>.
<Off>
Does not display the screen for confirming the fax number.
<On>
Displays the screen for confirming the fax number.

## Displaying Destinations in Address Book

When using coded dial numbers to specify destinations, you need to remember whose destination (or what group) is registered in what coded dial number. If you do not remember all these numbers perfectly, you may send your documents to unintended destinations. You can avoid sending data to unintended recipients by configuring the machine to display the details of the coded dial number you selected/entered as a sending destination before you send documents to that destination.
1
Tap <Menu> in the Home screen.
2
Tap <System Management Settings>.
If the logon screen appears, enter the correct ID and PIN using the numeric keys, and then press . Logging on to the Machine
3
Select <Restrict TX Function> <Coded Dial TX Confirmation>.
4
Tap <On>.
<Off>
Does not display the details of the entered coded dial number.
<On>
Displays the details of the entered coded dial number.
LINKS
Registering Destinations
Specifying from Address Book
Specifying from Address Book
Registering Destinations in the Address Book from Remote UI
0Y01-09A