# Network Settings

|  | All the settings about the network are listed with short descriptions. Default settings are marked with a dagger ().

##### Asterisks (*) Settings marked with an asterisk (*) cannot be imported or exported.

Select Wired/Wireless LAN
Wireless LAN Settings
Enable Direct Connection
TCP/IP Settings
SNMP Settings
Dedicated Port Settings
Waiting Time for Connection at Startup
Ethernet Driver Settings
IEEE 802.1X Settings
Device Settings Management On/Off
Initialize Network Settings

## Select Wired/Wireless LAN

When switching the machine from Wireless LAN to Wired LAN, you need to specify the setting. Conversely, when switching the machine from Wired LAN to Wireless LAN, you do not need to specify this setting (You can switch using the following <Wireless LAN Settings>). Selecting Wired LAN or Wireless LAN

Wired LAN Wireless LAN

## Wireless LAN Settings

Specify settings for connecting the machine to a wireless LAN. You can also view the current settings or specify the setting for saving power consumption.

##### WPS Push Button Mode

Select to automatically configure a wireless connection by using the button on a WPS wireless router. Setting Up Connection Using WPS Push Button Mode

##### WPS PIN Code Mode

Select to configure a wireless connection by entering a PIN code for a WPS wireless router. Setting Up Connection Using WPS PIN Code Mode

##### SSID Settings

Select to configure a wireless connection by specifying information including an SSID or a network key by inputting manually from the operation panel.

###### Select Access Point

Wireless LAN routers that can access the machine are automatically located, so you can select from the list. You must manually enter a network key, such as a WEP key or a PSK. Setting Up Connection by Selecting a Wireless Router

###### Enter Manually

Select to configure a wireless connection by manually entering an SSID. By using this method, you can specify authentication and encryption settings in detail. Setting Up Connection by Specifying Detailed Settings

Security Settings None WEP Open System WEP Key: 1/2/3/4 Edit WEP Key Shared Key WEP Key: 1/2/3/4 Edit WEP Key WPA/WPA2-PSK Auto AES-CCMP

##### Power Save Mode

Select whether or not the machine enters Power Save Mode based on signals emitted from the wireless router.

Off On

<Menu> <Network Settings> <Wireless LAN Settings> Read the displayed message <OK> <Power Save Mode> Select <Off> or <On>

##### Connection Information

Select to view the current wireless LAN settings. Viewing Network Settings

MAC Address Wireless LAN Status Latest Error Information Channel SSID Settings Security Settings Power Save Mode

## Enable Direct Connection *

Set whether to connect directly. By enabling this function, connecting directly with the machine is possible even in an environment without an access point or wireless LAN router.

Off On

<Menu> <Network Settings> <Enable Direct Connection> Select <Off> or <On> Restart the machine

Setting <Enable Direct Connection> to <On> prevents use of a wired LAN or any wireless LAN other than Direct Connection.

## TCP/IP Settings

Specify settings for using the machine in a TCP/IP network, such as IP address settings.

##### IPv4 Settings

Specify settings for using the machine in an IPv4 network.

###### IP Address Settings

Configure the IP address, which is used for identifying devices, such as computers and printers, on a TCP/IP network. Setting IPv4 Address

Auto Acquire Select Protocol Off DHCP Auto IP Off On Manually Acquire IP Address: 0.0.0.0 Subnet Mask: 0.0.0.0 Gateway Address: 0.0.0.0 Check Settings Auto Acquire IP Address Subnet Mask Gateway Address

###### PING Command

Select to check that the machine is connected to a computer over a network. Testing the Network Connection

###### DNS Settings

Specify settings for Domain Name System (DNS), which provides a host name for IP address resolutions. Configuring DNS

DNS Server Settings Primary DNS Server: 0.0.0.0 Secondary DNS Server: 0.0.0.0 DNS Host Name/Domain Name Settings Host Name Domain Name DNS Dynamic Update Settings Off On DNS Dynamic Update Interval 0 to 24 to 48 (hr.)

###### mDNS Settings

Specify settings for using DNS functions without DNS servers. Configuring DNS

Off On mDNS Name

###### DHCP Option Settings

If DHCP is enabled, use these settings to select whether to use the DHCP optional functions to acquire the DNS server address or the domain name. Configuring DNS

Acquire Host Name Off On DNS Dynamic Update Off On Acquire DNS Server Address Off On Acquire Domain Name Off On Acquire WINS Server Address Off On Acquire SMTP Server Address Off On Acquire POP Server Address Off On

##### IPv6 Settings

Specify settings for using the machine in an IPv6 network.

###### Use IPv6

Enable or disable IPv6 in the machine. You can also view the current settings. Setting IPv6 Addresses

Off On Check Settings Link-Local Address Prefix Length

###### Stateless Address Settings

Enable or disable stateless addresses. Setting IPv6 Addresses

Off On Check Settings Stateless Address Prefix Length

###### Use DHCPv6

Enable or disable the stateful address that is acquired via DHCPv6. Setting IPv6 Addresses

Off On Check Settings Stateful Address Prefix Length

###### DNS Settings

Specify settings for Domain Name System (DNS), which provides a host name for IP address resolutions. Configuring DNS

DNS Host Name/Domain Name Settings Use IPv4 Host/Domain Off Host Name Domain Name On DNS Dynamic Update Settings Off On Register Manual Address Off On Register Stateful Address Off On Register Stateless Address Off On DNS Dynamic Update Interval 0 to 24 to 48 (hr.)

###### mDNS Settings

Specify settings for using DNS functions without DNS servers. Configuring DNS

Off On Use Same mDNS Name as IPv4 Off mDNS Name On

###### DHCP Option Settings

If DHCP is enabled, use these settings to select whether to use the DHCP optional functions to acquire the DNS server address or the domain name. Configuring DNS

Acquire DNS Server Address Off On Acquire Domain Name Off On

##### WINS Settings

Specify settings for Windows Internet Name Service (WINS), which provides a NetBIOS name for IP address resolutions in a mixed network environment of NetBIOS and TCP/IP. Configuring WINS

WINS Resolution Off On WINS Server Address: 0.0.0.0

##### LPD Settings

Enable or disable LPD, a printing protocol that can be used on any hardware platform or operating system. You can also set the reception timeout period after which printing is canceled if print data reception is interrupted. Configuring Printing Protocols and WSD Functions

LPD Print Settings Off On RX Timeout 1 to 5 to 60 (min.)

##### RAW Settings

Enable or disable RAW, a Windows specific printing protocol. You can also set the reception timeout period after which printing is canceled if print data reception is interrupted. Configuring Printing Protocols and WSD Functions

RAW Print Settings Off On RX Timeout 1 to 5 to 60 (min.)

##### WSD Settings

Enable or disable automatic browsing and acquiring information for the printer or scanner by using the WSD protocol that is available on Windows Vista/7/8/Server 2008/Server 2012. Configuring Printing Protocols and WSD Functions

WSD Print Settings Use WSD Print Off On Use WSD Browsing Off On WSD Scan Settings Use WSD Scan Off On Use Computer Scan Off On Use Multicast Discovery Off On

##### Use FTP PASV Mode

Specify whether to use PASV mode for FTP. If you are connecting to an FTP server through a firewall, you must select PASV mode. Configuring FTP PASV mode

Off On

##### Use HTTP

Enable or disable HTTP, which is required for communications with a computer, such as when using the Remote UI, WSD printing, or printing with Google Cloud Print. Disabling HTTP Communication

Off On

##### Port Number Settings

Change port numbers for protocols according to the network environment. Changing Port Numbers

LPD 1 to 515 to 65535 RAW 1 to 9100 to 65535 WSD Multicast Discovery 1 to 3702 to 65535 HTTP 1 to 80 to 65535 Multicast Discovery 1 to 427 to 65535 POP3 1 to 110 to 65535 SMTP 1 to 25 to 65535 FTP 1 to 21 to 65535 SNMP 1 to 161 to 65535

##### MTU Size

Select the maximum size of packets the machine sends or receives. Changing the Maximum Transmission Unit

1300 1400 1500

## SNMP Settings

Specify the settings for monitoring and controlling the machine from a computer running SNMP-compatible software. Monitoring and Controlling the Machine with SNMP

##### SNMPv1 Settings

Enable or disable SNMPv1. When enabling SNMPv1, specify a community name and access privileges to Management Information Base (MIB) objects.

Off On

<Menu> <Network Settings> <SNMP Settings> <SNMPv1 Settings> Select <Off> or <On> Restart the machine

##### SNMPv3 Settings

Enable or disable SNMPv3. Use the Remote UI to specify detailed settings that are applied when SNMPv3 is enabled.

Off On

<Menu> <Network Settings> <SNMP Settings> <SNMPv3 Settings> Select <Off> or <On> Restart the machine

##### Acquire Printer Management Information from Host

Enable or disable the monitoring of printer management information from a networked computer running SNMP-compatible software.

Off On

<Menu> <Network Settings> <SNMP Settings> <Acquire Printer Management Information from Host> Select <Off> or <On> Restart the machine

## Dedicated Port Settings

Enable or disable the dedicated port. The dedicated port is used when printing, faxing, or scanning uses MF Scan Utility and when browsing or specifying the machine settings over the network.

Off On

<Menu> <Network Settings> <Dedicated Port Settings> Select <Off> or <On> Restart the machine

## Waiting Time for Connection at Startup

Specify a wait time for connecting to a network. Select the setting depending on the network environment. Setting a Wait Time for Connecting to a Network

0 to 300 (sec.)

## Ethernet Driver Settings

Select the Ethernet type (10BASE-T/100BASE-TX/1000BASE-T) and the communication mode of Ethernet (half-duplex/full-duplex). You can also view the MAC address for wired LAN.

##### MAC Address

Check the MAC address of the machine, which is a number unique to each communication device. Viewing the MAC Address for Wired LAN

##### Auto Detect

Select whether to automatically detect or manually select the communication mode and the Ethernet type. Configuring Ethernet Settings

Off Communication Mode Half Duplex Full Duplex Ethernet Type 10BASE-T 100BASE-TX 1000BASE-T On

## IEEE 802.1X Settings *

Enable or disable IEEE 802.1X authentication. Configuring IEEE 802.1X Authentication

Off On

<Menu> <Network Settings> <IEEE 802.1X Settings> Select <Off> or <On> Restart the machine

## Device Settings Management On/Off

Specify whether to use imageWARE Enterprise Management Console plug-ins to manage machine data such as settings and Address Book destinations. For detailed information on imageWARE Enterprise Management Console, contact your nearest Canon dealer.
<Menu> <Network Settings> <Device Settings Management On/Off> Select <Off> or <On>

Off On

## Initialize Network Settings

Select to return the Network Settings to the factory defaults. Initialize Menu
0Y01-0A9