# Print Mode

| All the settings about print mode switching are listed with short descriptions. Default settings are marked with a dagger ().

##### Asterisks (*) Settings marked with an asterisk (*) are not displayed depending on other settings or whether an optional ROM is installed on the machine.

Auto Mode Selection Auto Select Mode Priority

### Type of Print Mode

Auto selection mode | The machine enters the auto selection mode when <Auto Selection> is selected for <Auto Mode Selection>. The machine automatically discriminates data sent from a computer and selects the print mode. Normally use this print mode when you print from an application.
<PCL> | Mode for printing a PCL file sent from a computer.
<PS> | Mode for printing a PS file sent from a computer.
<PDF> | Mode for printing a PDF file by using Direct Print or USB Direct Print.
<XPS> | Mode for printing an XPS file by using Direct Print or USB Direct Print.

## Auto Mode Selection

Specify the print mode in which the machine operates.

Auto Selection PCL PS PDF XPS

() <Print Mode> <Auto Mode Selection> Select the print mode

## Auto Select

Enable or disable the automatic mode selection feature for the print modes during auto selection mode.

Off On

() <Print Mode> <Auto Select> Select the print mode <Off> or <On>

If all print modes are set to <Off>, the machine operates in the print mode specified for <Mode Priority>.

## Mode Priority

Specify the print mode that is automatically selected when the machine cannot identify the control command during auto selection mode.

None PCL PS PDF XPS

() <Print Mode> <Mode Priority> Select the preferential print mode

If you select <None>, the machine automatically determines the print mode when it cannot identify the control command.

101K-05K