# Specifying Settings via FTP Client

You can specify settings, such as the network settings of the machine, from an FTP client via TCP/IP network. Check the IP address set to the machine in advance (Network Status Print). If you are unsure of the IP address, contact your network administrator.
1
Start [Command Prompt].
Open the [Start] menu and select [All Programs] or [Programs] [Accessories] [Command Prompt].
For Mac OS users
Start the Terminal.
For UNIX users
Display the console screen.
2
Enter "ftp <IP address of the machine>" and press the [ENTER] key.
Example: ftp 192.168.1.45
3
Enter "root" for the user name and press the [ENTER] key.
4
Enter the System Manager password and press the [ENTER] key.
The default password is "7654321". Setting the System Manager Password
"230 User root logged in." is displayed.
5
Enter "cd config" and press the [ENTER] key.
6
Enter "get CONFIG <file name>" and press the [ENTER] key.
"CONFIG" must be all uppercase.
Any characters can be used in <file name> (example: get CONFIG Setting.txt).
The setting file is downloaded to the directory that is displayed when Command Prompt is started. In an example of a screen, the file is downloaded to the "USER_NAME" folder in [Users] on drive C:.
7
Edit the downloaded config file by using the text editor such as Notepad.

###### List of config file setting items

General Menu (General Settings)

Item Name | Setting Value | Factory Default Setting
DEVICE_NAME (Device Name) | Up to 128 characters | LBP712Cx/LBP710Cx
SYS_LOC (Location) | Up to 128 characters | (Blank)
SYS_CONTACT (System Manager) | Up to 128 characters | (Blank)
ROOT_PWD (System Manager Password) | Up to 16 alphanumeric characters | 7654321
USER_JOB_CONT (Allow End-User's Job Operation) | ON, OFF | OFF
LINK_URL1 (Support Link URL) | Up to 512 alphanumeric characters | http://www.canon.com

TCP/IP Menu (TCP/IP Settings)

Item Name | Setting Value | Factory Default Setting
INT_ADDR (IP Address) | IP Address | 0.0.0.0
NET_MASK (Subnet Mask) | IP Address | 0.0.0.0
DEF_GW (Gateway Address) | IP Address | 0.0.0.0
DHCP_ENB (Use DHCP) | ON, OFF | OFF
RARP_ENB (Use RARP) | ON, OFF | OFF
BOOTP_ENB (Use BOOTP) | ON, OFF | OFF
DNS_PADDR (Primary DNS Server Address) | IP Address | 0.0.0.0
DNS_SADDR (Secondary DNS Server Address) | IP Address | 0.0.0.0
HOST_NAME (Host Name) | Up to 47 alphanumeric characters | "Canon"+ "Lower 6 digits of MAC address"
DOMAIN_NAME (Domain Name) | Up to 47 alphanumeric characters | (Blank)
DDNS_ENB (DNS Dynamic Update) | ON, OFF | OFF
WINS_ENB (WINS Resolution) | ON, OFF | OFF
WINS_SERVER (WINS Server Address) | IP Address | 0.0.0.0
ARP_PING_ENB (Use ARP/PING) | ON, OFF | ON
LPD_ENB (Use LPD Printing) | ON, OFF | ON
LPD_BANN (Print LPD Banner Page) | ON, OFF | OFF
RAW_ENB (Use RAW Printing) | ON, OFF | ON
RAW_BIDIR_ENB (Use Bidirectional Communication) | ON, OFF | OFF
FTP_PRINT_ENB (Use FTP Print) | ON, OFF | OFF
FTP_PRINT_USER (FTP Print User Name) | Up to 24 alphanumeric characters | guest
FTP_PRINT_PWD (FTP Print Password) | Up to 24 alphanumeric characters | 7654321
IPP_ENB (Use IPP) | ON, OFF | ON
IPP_AUTH_ENB (Use IPP Authentication) | ON, OFF | OFF
IPP_AUTH_ACCUNT1 (IPP Authentication User Name) | Up to 24 alphanumeric characters (mandatory when using IPP authentication) | guest
IPP_AUTH_PASSWD1 (IPP Authentication Password) | Up to 24 alphanumeric characters (mandatory when using IPP authentication) | 7654321
WSD_ENB (Use WSD Printing) | ON, OFF | OFF
WSD_BROWSING (Use WSD Browsing) | ON, OFF | OFF
WSD_MULTICAST_ DISCOVERY (Use Multicast Discovery) | ON, OFF | OFF
HTTP_ENB (Use HTTP) | ON, OFF | ON
SNTP_ENB (Use SNTP) | ON, OFF | OFF
SNTP_ADDR (NTP Server Name) | IP address or host name | (Blank)
SNTP_INTERVAL (Polling Interval) | 1 to 48 (hr.) | 24
DISCOVERY_ENB (Respond to Discovery) | ON, OFF | ON
DISCOVERY_SCOPE_NAME (Scope Name) | Up to 32 alphanumeric characters | default
EMAIL_PRINT_ENB (POP3 RX) | ON, OFF | OFF
EMAIL_POP_ADDR (POP3 Server Name) | Up to 48 alphanumeric characters | (Blank)
EMAIL_POP_ACCOUNT (POP3 User Name) | Up to 32 alphanumeric characters | (Blank)
EMAIL_POP_PASSWD (POP3 Password) | Up to 32 alphanumeric characters | (Blank)
EMAIL_POP_INTERVAL (POP3 RX Interval) | 0 to 90 (min.) | 0
EMAIL_POP_PORTNO (POP3 Server Port Number) | 0 to 65535 | 110
IPV4_USE (Use IPv4) | ON, OFF | ON
IPV6_USE (Use IPv6) | ON, OFF | OFF
IPV6_STATELESS_USE (Use Stateless Address) | ON, OFF | ON
IPV6_MANUAL_ADDR_USE (Use Manual Address) | ON, OFF | OFF
IPV6_MANUAL_ADDR_SET (IP Address) | IP Address | (Blank)
IPV6_MANUAL_ADDR_PREFIX (Prefix Length) | 0 to 128 | 64
IPV6_MANUAL_ROUTER_ADDR (Default Router Address) | IP Address | (Blank)
IPV6_DHCPV6_USE (Use DHCPv6) | ON, OFF | OFF
IPV6_DNS_ADDRESS_PRI (Primary DNS Server Address) | IP Address | (Blank)
IPV6_DNS_ADDRESS_SEC (Secondary DNS Server Address) | IP Address | (Blank)
IPV6_DNS_NAME_ SAME_AS_IPV4 (Use IPv4 Host/Domain Names) | ON, OFF | OFF
IPV6_DNS_HOST_NAME_V6 (Host Name) | Up to 47 alphanumeric characters | "Canon"+ "Lower 6 digits of MAC address"
IPV6_DNS_DOMAIN_ NAME_V6 (Domain Name) | Up to 47 alphanumeric characters | (Blank)
IPV6_DNS_DYNAMIC_SET (DNS Dynamic Update) | ON, OFF | OFF
IPV6_DNS_STATELESS (Register Stateless Address) | ON, OFF | OFF
IPV6_DNS_MANUAL (Register Manual Address) | ON, OFF | OFF
IPV6_DNS_STATEFUL (Register Stateful Address) | ON, OFF | OFF

SMB Server Menu (SMB Settings)

Item Name | Setting Value | Factory Default Setting
SMB_ENB (Use SMB) | ON, OFF | OFF
SMB_SERVER (Server Name) | Up to 16 characters | (Blank)
SMB_WG (Workgroup Name) | Up to 16 characters | WORKGROUP
SMB_COMMENT (Comments) | Up to 192 characters | (Blank)
SMB_LM_ENB (Use LM Announce) | ON, OFF | OFF
SMB_PRINT_ENB (Use SMB Printing) | ON, OFF | OFF
SMB_PRINTER (Printer Name) | Up to 13 characters | PRINTER

SNMP Menu (SNMP Settings)

Item Name | Setting Value | Factory Default Setting
SNMP_V1_ENB (Use SNMPv1) | ON, OFF | ON
SNMP_COMMUNITY1_ ENB (Use Community Name 1) | ON, OFF | ON
SNMP_COMMUNITY1_ ACCESS (MIB Access Permission) | RW (Read/Write), RO (Read Only) | RO
SNMP_COMMUNITY1_ NAME (Community Name 1) | Up to 32 alphanumeric characters | public
SNMP_COMMUNITY2_ ENB (Use Community Name 2) | ON, OFF | OFF
SNMP_COMMUNITY2_ ACCESS (MIB Access Permission) | RW (Read/Write), RO (Read Only) | RO
SNMP_COMMUNITY2_ NAME (Community Name 2) | Up to 32 alphanumeric characters | public2
SNMP_V3_ENB (Use SNMPv3) | ON, OFF | OFF
SNMP_GET_PRT_MNG_ INFO (Obtain Printer Management Information from Host) | ON, OFF | OFF

SPOOLER Menu (Spool Settings)

Item Name | Setting Value | Factory Default Setting
SPOOL_ENB (Use Spooler) | ON, OFF | OFF

START TIMER Menu (Waiting Time Settings for Connection at Startup)

Item Name | Setting Value | Factory Default Setting
STRT_DELAY_TIME (Waiting Time for Connection at Startup) | 0 to 300 (sec.) | 0

RUI Menu (Remote UI Settings)

Item Name | Setting Value | Factory Default Setting
RUI_ENB (Use Remote UI) | ON, OFF | ON

8
Enter "put <file name> CONFIG" and press the [ENTER] key.
Specify the edited file name in <file name> (example: put Setting.txt CONFIG).
The setting file is uploaded.
9
Enter "get reset" and press the [ENTER] key.
The machine is restarted. The settings are enabled after the machine is restarted.
10
Confirm that the machine has been normally restarted, press [C] key while holding down the [CTRL] key.
11
Enter "quit" and press the [ENTER] key.
12
Enter "exit" and press the [ENTER] key.
Command Prompt exits.
LINKS
Network
101K-08A