# Interface

| All the settings about interfaces for communications with a computer and USB are listed with short descriptions. Default settings are marked with a dagger ().

##### Asterisks (*) Settings marked with an asterisk (*) are not displayed depending on other settings.

Interface Selection Timeout Connection Recog. Extended RX Buffer

## Interface Selection

Select the interface used for the machine.

##### USB

Enable or disable the USB port. Restricting the USB Connection with a Computer

Off On

##### Network

Enable or disable the LAN port. Disabling the LAN Port

Off On

##### USB Adv. Functions

Specify settings for selecting a function to use a USB device or selecting a device driver to use.

###### Adv. Func. Settings

Select which of MEAP applications and USB over NW to be given priority when a USB device is connected to the machine.

Meap Priority USB Over NW Priority

() <Interface> <Interface Selection> Check the message <USB Adv. Functions> <Adv. Func. Settings> <Meap Priority> or <USB Over NW Priority> Perform a hard reset (Performing a Hard Reset)

#### <Meap Priority>

Specify this to give priority to MEAP applications.

#### <USB Over NW Priority>

Specify this to give priority to USB over NW. This function enables you to use, from your computer, a USB device connected to the machine's USB port.

###### USB Storage Device

Specify settings for the device driver for using a USB memory device.
MEAP Driver
Enable or disable the MEAP specific device driver when a USB memory device is attached to the machine. When you want to perform the direct print function (USB Direct Print) from a USB memory device without using a computer, select <Off>.

Off On

() <Interface> <Interface Selection> Check the message <USB Adv. Functions> <USB Storage Device> <MEAP Driver> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Timeout

Specify how the machine should behave if receiving print data is interrupted.

##### Timeout

Select whether to cancel printing if print data receiving is interrupted for a specified period of time.

Off On

() <Interface> <Timeout> <Timeout> <Off> or <On>

##### Timeout Time *

Set the time period until a timeout error occurs.

5 to 15 to 300 (seconds)

() <Interface> <Timeout> <Timeout Time> Use the numeric keys to set the time period

## Connection Recog.

A problem such as improper overlay printing or garbled characters may occur during printing via wired LAN connection. In this case, set <Connection Recog.> to <Off>.

Off On

() <Interface> <Connection Recog.> Check the message <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Extended RX Buffer

Select whether to increase the space of the memory built in the machine for receiving print data from a computer. If you select <On>, the time until the computer will be freed from print data processing or transmission can be reduced when the computer sends a large volume of data or complicatedly structured data.

Off On

() <Interface> <Extended RX Buffer> Check the message <Off> or <On> Perform a hard reset (Performing a Hard Reset)
101K-05H