# Exterior

Regularly wipe the exterior of the machine, especially around the ventilation slots, to keep the machine in good condition.
1
Turn OFF the machine, and unplug the power cord from the AC power outlet.
When you turn OFF the power, shut down the machine from the operation panel without using the power switch. Turning OFF the Power (Performing a Shutdown)
2
Clean the exterior of the machine and the ventilation slots.
Use a soft, well-wrung-out cloth dampened with water or a mild detergent diluted with water.
To locate the ventilation slots, see Front Side and Back Side.
3
Wait for the exterior of machine to dry completely.
4
Reconnect the power cord and turn ON the machine.
101K-06U