# Network

| All the settings about the network are listed with short descriptions. Default settings are marked with a dagger ().

##### If <Network> is not displayed If <Network> under <Interface Selection> is set to <Off>, <Network> is not displayed in the Setup menu. Interface Selection ##### Asterisks (*) Settings marked with an asterisk (*) are not displayed depending on other settings or whether an optional SD card is installed on the machine.

TCP/IP Settings Mopria Google Cloud Print SMB SNMP Settings Spooler Receive in Parallel Wait Time at Startup |  | Remote UI Settings Ethernet Driver Sleep Mode Priority IEEE802.1X Address Filter MAC Address E-Mail Print Set. Init. Network Set.

## TCP/IP Settings

Specify settings for using the machine in a TCP/IP network, such as IP address settings.

##### IPv4 Settings

Specify settings for using the machine in an IPv4 network.

###### IPv4

Enable or disable IPv4 in the machine.

Off On

() <Network> Check the message <TCP/IP Settings> <IPv4 Settings> <IPv4> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### IP Mode

Select how to set the IP address. Setting IPv4 Address

Auto Manual

###### Protocol *

Select the protocol to use when <IP Mode> is set to <Auto>. If you set the selected protocol to <On>, the other two protocols are automatically set to <Off>. Setting IPv4 Address
Use DHCP

Off On

Use BOOTP

Off On

Use RARP

Off On

###### Auto IP *

Select whether to automatically obtain an IP address. Specify <On> when <IP Mode> is set to <Auto>. Setting IPv4 Address

Off On

###### IP Address Settings

Configure the IP address, which is used for identifying devices, such as computers and printers, on a TCP/IP network. Setting IPv4 Address
IP Address

0.0.0.0 to 255.255.255.255

Subnet Mask

0.0.0.0 to 255.255.255.255

Gateway Address

0.0.0.0 to 255.255.255.255

###### DNS

Specify settings for the server address of the Domain Name System (DNS), which provides a host name for IP address resolutions. Use / to move the cursor, and use the numeric keys to specify the address. Use the Remote UI to specify other settings for DNS. Configuring DNS
Primary Address

0.0.0.0 to 255.255.255.255

Secondary Address

0.0.0.0 to 255.255.255.255

() <Network> Check the message <TCP/IP Settings> <IPv4 Settings> <DNS> Select the server to configure Set the address Perform a hard reset (Performing a Hard Reset)

###### mDNS Settings *

Specify settings for using DNS functions without DNS servers. Configuring DNS
mDNS

Off On

() <Network> Check the message <TCP/IP Settings> <IPv4 Settings> <mDNS Settings> <mDNS> <Off> or <On> Perform a hard reset (Performing a Hard Reset)
mDNS Name *
When <mDNS> is set to <On>, set this item.
() <Network> Check the message <TCP/IP Settings> <IPv4 Settings> <mDNS Settings> <mDNS Name> Set the name Perform a hard reset (Performing a Hard Reset)

###### DHCP Option

When DHCP is enabled, select whether to acquire the host name and whether to perform dynamic update of the DNS using the DHCP options.
Acquire Host Name

Off On

DNS Dynamic Update

Off On

() <Network> Check the message <TCP/IP Settings> <IPv4 Settings> <DHCP Option> <Acquire Host Name> or <DNS Dynamic Update> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### IPv6 Settings

Select whether to use the machine in an IPv6 network. Use the Remote UI to specify the IPv6 address settings. Setting IPv6 Addresses

###### IPv6

Enable or disable IPv6 in the machine.

Off On

() <Network> Check the message <TCP/IP Settings> <IPv6 Settings> <IPv6> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### mDNS Settings *

Specify settings for using DNS functions without DNS servers. Configuring DNS
mDNS

Off On

() <Network> Check the message <TCP/IP Settings> <IPv6 Settings> <mDNS Settings> <mDNS> <Off> or <On> Perform a hard reset (Performing a Hard Reset)
Use IPv4 Name (mDNS) *

Off On

() <Network> Check the message <TCP/IP Settings> <IPv6 Settings> <mDNS Settings> <Use IPv4 Name (mDNS)> <Off> or <On> Perform a hard reset (Performing a Hard Reset)
mDNS Name *
When <Use IPv4 Name (mDNS)> is set to <Off>, set this item.
() <Network> Check the message <TCP/IP Settings> <IPv6 Settings> <mDNS Settings> <mDNS Name> Set the name Perform a hard reset (Performing a Hard Reset)

##### WINS Resolution

Select whether to use Windows Internet Name Service (WINS), which provides a NetBIOS name for IP address resolutions in a mixed network environment of NetBIOS and TCP/IP. Use the Remote UI to specify detailed settings that are applied when WINS is enabled. Configuring WINS

Off On

() <Network> Check the message <TCP/IP Settings> <WINS Resolution> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### FTP

Select whether to change the settings for printing and those configured in the machine from FTP.

###### FTP Print

Select whether to print from FTP. Use the Remote UI to set the user name and password that are used to print from FTP. Preparing for Using the FTP Server

Off On

() <Network> Check the message <TCP/IP Settings> <FTP> <FTP Print> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### Allow Set. via FTP

Select whether to change the settings configured in the machine from FTP.

Off On

() <Network> Check the message <TCP/IP Settings> <FTP> <Allow Set. via FTP> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### LPD Settings

Enable or disable LPD, a printing protocol that can be used on any hardware platform or operating system. Also, set the time period after which the print job automatically ends when print data cannot be received due to a communication error or some other problem. Use the Remote UI to specify settings for banner page printing when LPD is enabled. Configuring Printing Protocols and WSD Functions

###### LPD Print

Off On

() <Network> Check the message <TCP/IP Settings> <LPD Settings> <LPD Print> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### RX Timeout *

1 to 60 (min.)

() <Network> Check the message <TCP/IP Settings> <LPD Settings> <RX Timeout> Set Timeout Time Perform a hard reset (Performing a Hard Reset)

##### RAW Settings

Enable or disable RAW, a Windows specific printing protocol. Also, set the time period after which the print job automatically ends when print data cannot be received due to a communication error or some other problem. Use the Remote UI to specify settings for bidirectional communication. Configuring Printing Protocols and WSD Functions

###### RAW Print

Off On

() <Network> Check the message <TCP/IP Settings> <RAW Settings> <RAW Print> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### RX Timeout *

1 to 60 (min.)

() <Network> Check the message <TCP/IP Settings> <RAW Settings> <RX Timeout> Set Timeout Time Perform a hard reset (Performing a Hard Reset)

##### IPP Print

Enable or disable IPP, which enables printing from an external network via Internet. Use the Remote UI to specify settings for TLS encryption of data to send and user authentication. Configuring Printing Protocols and WSD Functions

Off On

() <Network> Check the message <TCP/IP Settings> <IPP Print> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### WSD

Enable or disable automatic browsing and acquiring information for the machine by using the WSD protocol that is available on Windows Vista/7/8/10/Server 2008/Server 2012. Configuring Printing Protocols and WSD Functions

###### WSD Print

Select whether to print with the machine by using WSD.

Off On

() <Network> Check the message <TCP/IP Settings> <WSD> <WSD Print> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### WSD Browsing *

Select whether to acquire information of the machine from a computer by using WSD. If <WSD Print> is set to <On>, <WSD Browsing> is fixed to <On> and is not displayed in the setting menu.

Off On

() <Network> Check the message <TCP/IP Settings> <WSD> <WSD Browsing> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### Multicast Discovery

Select whether to set the machine to reply to multicast discovery messages.

Off On

() <Network> Check the message <TCP/IP Settings> <WSD> <Multicast Discovery> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

If <Multicast Discovery> is set to <Off>, the machine stays in sleep mode even when multicast discovery messages are flowing on the network.

##### HTTP

Enable or disable HTTP. HTTP is required for communications with a computer, such as when using the Remote UI and performing WSD printing. Disabling HTTP Communication

Off On

##### Proxy Settings

Specify settings for using the proxy server that relays HTTP communications. Setting a Proxy

###### Proxy

Enable or disable the proxy server when the machine performs HTTP communications.

Off On

() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <Proxy> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### Server Address *

Set the address of the proxy server to use. Specify the IP address, domain name, and other necessary information that suit your operational environment. Use / to move the cursor, and use the numeric keys to enter the address (Entering Text).
() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <Server Address> Enter the server address Perform a hard reset (Performing a Hard Reset)

###### Port Number *

Specify the port number of the proxy server to use.

1 to 80 to 65535

() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <Port Number> Enter the port number Perform a hard reset (Performing a Hard Reset)

###### Same Domain *

Enable or disable the proxy server even for performing HTTP communications with devices in the same domain.

Use Proxy Do Not Use Proxy

() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <Same Domain> <Use Proxy> or <Do Not Use Proxy> Perform a hard reset (Performing a Hard Reset)

###### Proxy Authentication *

Enable or disable the authentication function of the proxy server.

Off On

() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <Proxy Authentication> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### User Name *

To enable the proxy authentication, enter up to 24 alphanumeric characters for the user name to authenticate. Use the numeric keys to enter the user name. (Entering Text)
() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <User Name> Enter the user name Perform a hard reset (Performing a Hard Reset)

###### Password *

To set the password for the proxy authentication, enter up to 24 alphanumeric characters. Use the numeric keys to enter the password. (Entering Text)
() <Network> Check the message <TCP/IP Settings> <Proxy Settings> <Password> Enter the password Perform a hard reset (Performing a Hard Reset)

##### SNTP

Select whether to acquire time from a network time server. Use the Remote UI to specify the server address settings. Configuring SNTP

Off On

() <Network> Check the message <TCP/IP Settings> <SNTP> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### Discovery Response

Select whether to set the machine to respond to multicast discovery packets on the network. Use the Remote UI to specify the scope name that is used to include the machine into a specific scope. Configuring Settings for Device Management Software

Off On

() <Network> Check the message <TCP/IP Settings> <Discovery Response> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### IPSec

Select whether to perform encrypted communication by establishing a virtual private network (VPN) via IPSec. Use the Remote UI to register and specify the security policies. Configuring IPSec Settings

Off On

() <Network> Check the message <TCP/IP Settings> <IPSec> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### Sleep Notif. Set.

Specify settings for SLP communication to notify imageWARE of the power status of the machine. If you set <Sleep Mode Notif.> to <On>, you can expect the machine to avoid unnecessary communication during sleep mode and reduce the total power consumption. Configuring Settings for Device Management Software

###### Sleep Mode Notif.

Enable or disable SLP communication. If you select <On>, the power status of the machine is notified to imageWARE.

Off On

() <Network> Check the message <TCP/IP Settings> <Sleep Notif. Set.> <Sleep Mode Notif.> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### Port Number *

Enter the port number for SLP communications with management software.

1 to 11427 to 65535

() <Network> Check the message <TCP/IP Settings> <Sleep Notif. Set.> <Port Number> Use the numeric keys to enter the port number Perform a hard reset (Performing a Hard Reset)

###### Routers to Traverse *

Specify how many routers the notification packets can pass. Enter a number from 0 to 254.

0 to 3 to 254

() <Network> Check the message <TCP/IP Settings> <Sleep Notif. Set.> <Routers to Traverse> Use the numeric keys to enter the number of routers to traverse Perform a hard reset (Performing a Hard Reset)

###### Notif. Interval *

Specify how often the machine notifies imageWARE of its power status. Enter a number in seconds from 60 to 65535.

60 to 600 to 65535

() <Network> Check the message <TCP/IP Settings> <Sleep Notif. Set.> <Notif. Interval> Use the numeric keys to enter the notification interval Perform a hard reset (Performing a Hard Reset)

## Mopria

Select whether to use Mopria®. Printing with Mopria®

Off On

() <Network> Check the message <Mopria> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Google Cloud Print

Enable or disable Google Cloud Print. Changing Google Cloud Print Settings

Use Cloud Print Off On Registration Status

## SMB *

Select whether to use the machine as a shared printer on the SMB network. Use the Remote UI to specify other SMB settings including the server name and the workgroup name. Configuring SMB

##### SMB Server

Select whether to display the machine as an SMB Server on the SMB network configuration screen.

Off On

() <Network> Check the message <SMB> <SMB Server> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### SMB Print *

Enable or disable SMB Print.

Off On

() <Network> Check the message <SMB> <SMB Print> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## SNMP Settings

Specify the settings for monitoring and controlling the machine from a computer running SNMP-compatible software. Monitoring and Controlling the Machine with SNMP

##### SNMPv1 Settings

Specify settings for using SNMPv1. Use the Remote UI to specify a community name and access privileges to Management Information Base (MIB) objects.

###### SNMPv1

Enable or disable SNMPv1.

Off On

() <Network> Check the message <SNMP Settings> <SNMPv1 Settings> <SNMPv1> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### Dctd. Community Set.

Dedicated Community is a preset community, intended exclusively for administrators using Canon software, such as imageWARE Enterprise Management Console. Select the access privilege to Management Information Base (MIB) objects.
Dctd. Community

Off Read/Write Read Only

() <Network> Check the message <SNMP Settings> <SNMPv1 Settings> <Dctd. Community Set.> <Dctd. Community> Select the access privilege Perform a hard reset (Performing a Hard Reset)

##### SNMPv3 Settings

Specify settings for using SNMPv3. Use the Remote UI to specify detailed settings that are applied when SNMPv3 is enabled.

###### SNMPv3

Enable or disable SNMPv3.

Off On

() <Network> Check the message <SNMP Settings> <SNMPv3 Settings> <SNMPv3> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

###### User Settings N (N=1, 2, 3, 4, 5) *

Specify the authentication password and encryption password as the user information used on SNMPv3. Use the Remote UI to register the user information. Monitoring and Controlling the Machine with SNMP
Auth. Password/Encryption Password
Enter 6 to 16 alphanumeric characters for each password. Use the numeric keys to enter the password.
() <Network> Check the message <SNMP Settings> <SNMPv3 Settings> Select the user settings number Check the user name <Auth. Password> or <Encryption Password> Enter the password Perform a hard reset (Performing a Hard Reset)

##### Rjct Packet in Sleep

Select whether to discard SNMP packets received during sleep mode.

Off On

() <Network> Check the message <SNMP Settings> <Rjct Packet in Sleep> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

If you select <On>, applications that use the SNMP protocol, such as Canon software imageWARE Series, may be disabled to access the machine.

## Spooler *

Select whether to include the SD card in the storage locations of received print data. If you select <On>, the machine capacity of receiving print data is increased.

Off On

() <Network> Check the message <Spooler> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Receive in Parallel

Specifies whether to print jobs in the order received when print data for several jobs are sent to the printer from one computer. If you select <Off>, jobs are printed in the order received but printing speed may be slower.

Off On

() <Network> Check the message <Receive in Parallel> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Wait Time at Startup

Specify a wait time for connecting to a network. Select the setting depending on the network environment. Setting a Wait Time for Connecting to a Network

0 to 300 (sec.)

## Remote UI Settings

Specify settings for using the Remote UI. You can use the Remote UI to specify settings for the machine from a Web browser.

##### Remote UI

Enable or disable the Remote UI. Disabling Remote UI

Off On

##### RUI Access Sec. Set.

Set a PIN of up to 7 digits for access to the Remote UI. All users use a common PIN. Setting a Remote UI PIN

Off On Remote UI Access PIN

##### TLS *

Enable or disable TLS for Remote UI communications. To use TLS for encrypted communications, you need to set key pairs by using the Remote UI (Using TLS for Encrypted Communications), respectively.

Off On

() <Network> Check the message <Remote UI Settings> <TLS> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Ethernet Driver

Specify the Ethernet communication mode (half duplex/full duplex) and Ethernet type (10 Base-T/100 Base-TX/1000 Base-T). Configuring Ethernet Settings

##### Auto Detect

Select whether to automatically detect or manually select the communication mode and the Ethernet type.

Off On

##### Communication Mode *

If <Auto Detect> is set to <Off>, select the Ethernet communication mode.

Half Duplex Full Duplex

##### Ethernet Type *

If <Auto Detect> is set to <Off>, select the Ethernet type.

10 Base-T 100 Base-TX 1000 Base-T

## Sleep Mode Priority

Select whether to give priority to rapid returning from sleep mode or greater energy saving effect of sleep mode.

Optimal Balance Exit Speed Energy Saving

() <Network> Check the message <Sleep Mode Priority> Select the settings item Perform a hard reset (Performing a Hard Reset)

#### Optimal Balance

The machine returns from sleep mode rapidly. When the devices directly connected to the machine support EEE (Energy Efficient Ethernet), power consumption can be reduced to a greater degree. Normally use this setting.

#### Exit Speed

The machine returns from sleep mode more rapidly.

#### Energy Saving

Communication speed during sleep mode is reduced for lowest power consumption.

This item is available when <Sleep Mode> is set to <High (Deep Sleep)>. Entering Sleep Mode

## IEEE802.1X

Enable or disable IEEE 802.1X authentication. Use the Remote UI to specify detailed settings that are applied when IEEE802.1X authentication is enabled. Configuring IEEE 802.1X Authentication

Off On

() <Network> Check the message <IEEE802.1X> Check the message <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Address Filter

Enable or disable communication restricted with the IP address and MAC address. Use the Remote UI to specify the address to restrict. Basic Printing Operations

Off On

() <Network> Check the message <Address Filter> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## MAC Address

Check the MAC address of the machine, which is a number unique to each communication device.

(Display only)

() <Network> Check the message <MAC Address>

## E-Mail Print Set.

Specify settings for using the E-Mail Print function. Use the Remote UI to specify other settings for E-Mail Print including the mail server settings. Printing Received E-mail (E-Mail Print)

##### POP3 RX Interval

Specify the interval for automatically connecting to the mail server in minutes. New e-mails in the mailbox of the mail server are automatically received and printed at the specified time intervals.

0 to 90 (min.)

() <Network> Check the message <E-Mail Print Set.> <POP3 RX Interval> Use the numeric keys to enter the interval of auto e-mail reception Perform a hard reset (Performing a Hard Reset)

If you select "0," e-mails are not automatically received. In this case, receive e-mails manually. Manually Receiving E-Mails

##### POP3 RX

Enable or disable E-Mail Print for the POP3 mail server.

Off On

() <Network> Check the message <E-Mail Print Set.> <POP3 RX> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

##### SMTP RX

Enable or disable E-Mail Print for the SMTP protocol.

Off On

() <Network> Check the message <E-Mail Print Set.> <SMTP RX> <Off> or <On> Perform a hard reset (Performing a Hard Reset)

## Init. Network Set.

Select to return the Network Settings to the factory defaults. Initializing the Network Settings
101K-05C