# Relocating the Machine

The machine is heavy. Make sure to follow the procedures below when moving the machine to avoid injury, and also make sure to read the safety precautions before you begin. Important Safety Instructions
1
Turn OFF the machine and computer.
When you turn OFF the power, be sure to shut down the machine from the operation panel without using the power switch. Turning OFF the Power (Performing a Shutdown)
2
Disconnect the cables and cord from the machine in numerical order as in the illustration below.
Whether the cables with "*" are connected depends on your environment.

Power plug Power cord USB device* USB cable* LAN cable* |

3
When transporting the machine across a long distance, remove the toner cartridge. How to Replace Toner Cartridges
4
Pull out the paper drawer until it stops, and remove it while lifting the front side.
5
Close all the open covers, and move the machine to a new location.
The machine is heavy (Machine Specifications). Do not try hard to carry the machine.
Use the handles on both sides of the machine, and have at least two people carry it.
If the optional paper feeder is attached to the machine
Unlock the paper feeder before lifting the machine, and transport the paper feeder separately.
6
Carefully place the machine at the new installation site.
For information about how to install the machine after relocating it, see Getting Started. Manuals Included with the Machine
101K-070