# Configuring Settings for Device Management Software

You can facilitate the collection and management of various information about networked devices by implementing device management software, such as imageWARE Enterprise Management Console, into the network. Information such as device settings and error logs is retrieved and distributed via the server computer. If the machine is connected to such a network, imageWARE Enterprise Management Console searches the network for the machine by using protocols such as Service Location Protocol (SLP) to gather information from the machine, including the power status. SLP settings can be specified via the Remote UI.
1
Start the Remote UI and log on in Management Mode. Starting Remote UI
2
Click [Settings/Registration].
3
Click [Network] [TCP/IP Settings].
4
Specify SLP settings.

###### Specifying multicast device discovery

1 | Click [Edit] in [Multicast Discovery Settings].
2 | Select the [Respond to Discovery] check box and specify the required settings. [Respond to Discovery] Select the check box to set the machine to respond to device management software multicast discovery packets and enable monitoring by device management software. If you do not want to set the machine to respond, clear the check box. [Scope Name] To include the machine into a specific scope, enter up to 32 characters for the scope name.
3 | Click [OK].

###### Notifying a device management software of the power status of the machine

1 | Click [Edit] in [Sleep Mode Notification Settings].
2 | Select the [Notify] check box and specify the required settings. [Notify] Select the check box to notify a device management software of the power status of the machine. When [Notify] is selected, you can expect the machine to avoid unnecessary communication during sleep mode and reduce the total power consumption. [Port Number] Change the port number for this function according to the network environment. [Number of Routers to Traverse] Specify how many routers the notification packets can pass. Enter a number from 0 to 254. [Notification Interval] Specify how often the machine notifies a device management software of its power status. Enter a number in seconds from 60 to 65535.
3 | Click [OK].

5
Perform a hard reset.
Click [Device Control], select [Hard Reset], and then click [Execute].
The settings are enabled after the hard reset is performed.

##### Using the operation panel You can also enable or disable discovery response from the setting menu of the operation panel. Discovery Response Power status notification settings can also be accessed from the setting menu of the operation panel. Sleep Notif. Set.

LINKS
Entering Sleep Mode
101K-03K