# Machine Specifications

Hardware Specifications
Controller Specifications
Software Specifications

## Hardware Specifications

Type | Desktop page printer
Printing Method | Semiconductor laser + dry-type electrophotographic method
Toner Fixing System | On-demand fixing system
Resolution | 600 dpi
Print Speed *1 (Plain paper (60 to 90 g/m²), A4 continuous printing) | LBP712Cx Black and white printing 1-sided printing: 38 sheets/minute 2-sided printing: 38 pages/minute *2 Color printing 1-sided printing: 38 sheets/minute 2-sided printing: 38 pages/minute *2 LBP710Cx Black and white printing 1-sided printing: 33 sheets/minute 2-sided printing: 33 pages/minute *2 Color printing 1-sided printing: 33 sheets/minute 2-sided printing: 33 pages/minute *2
Warm-Up Time *3 (from power ON until machine enters standby) | Normal start: 31 seconds or less Quick start: 2 seconds or less
Recovery Time *4 (recovery from sleep mode to standby) | Mid (Printer Sleep): 6 seconds or less High (Deep Sleep): 6 seconds or less
First Print Time *4 (1-sided printing on A4 size paper, with the output tray used) | Black and white printing: 5.1 seconds Color printing: 6.0 seconds
Acceptable Paper Stock | Paper
2-Sided Printing | Standard size: A4, B5, A5, Legal, Letter, Executive, Foolscap, 16K, Indian Legal, Government Legal, Government Letter, and Australia Foolscap Custom paper size: Width 148.0 to 215.9 mm, Length 210.0 to 355.6 mm
Paper Output | Face down
Output Capacity *5 (Output Tray) | Approx. 200 sheets
Noise (measured in accordance with ISO 7779, declared noise emission in accordance with ISO 9296) | LwAd (Declared A-weighted sound power level (1 B = 10 dB)) During standby mode: LBP712Cx 5.0 B or less LBP710Cx 5.1 B or less During printing: LBP712Cx Black and white printing: 1-sided printing: 6.5 B or less 2-sided printing: 6.7 B or less Color printing: 1-sided printing: 6.6 B or less 2-sided printing: 6.7 B or less LBP710Cx Black and white printing: 1-sided printing: 6.5 B or less 2-sided printing: 6.7 B or less Color printing: 1-sided printing: 6.5 B or less 2-sided printing: 6.7 B or less LpAm (Declared A-weighted sound pressure level (Bystander position)) During standby mode: LBP712Cx 36 dB LBP710Cx 37 dB During printing: Black and white printing: 1-sided printing: 50 dB 2-sided printing: 52 dB Color printing: 1-sided printing: 51 dB 2-sided printing: 52 dB
Environmental Conditions (Main unit only) | System requirements Temperature: 10 to 30 °C Humidity: 20 to 80% RH (no condensation)
Power Supply | 220 to 240 V (± 10 %), 50/60 Hz (± 2 Hz)
Power Consumption *6 (at 20 °C) | Maximum: 1,470 W or less During operation: Approx. 590 W (LBP712Cx) Approx. 570 W (LBP710Cx) During standby: Approx. 34 W During sleep mode: <Mid (Printer Sleep)> *7: Approx. 6.1 W (Wired LAN connection) <High (Deep Sleep)> *7: Approx. 1.3 W (Wired LAN connection) During power-off: 0.16 W or less (shutdown) 0.84 W or less (quick turn-OFF)
Consumables | Consumables
Weight *8 | Approx. 24.8 kg

*1 The print speed may be slower depending on the output resolution, paper size, paper type, paper orientation, and a specified number of sheets to print. *2 For 2-sided printing, one page printed on the front side of a sheet and one printed on the back side are counted as one output sheet. *3 May vary depending on the use conditions of the machine (including attached optional accessories and installation environment). *4 May vary depending on the output environment. *5 May vary depending on the installation environment and paper type used. *6 Even if the printer is turned OFF, power is still consumed slightly while the power plug is inserted in the AC power outlet. To stop the power consumption completely, unplug the power plug from the AC power outlet. *7 Power may be consumed more than the values shown here according to the situation even if the sleep mode is set to <Mid (Printer Sleep)> or <High (Deep Sleep)>. *8 The weight of the machine excluding the weight of a toner cartridge.

## Controller Specifications

CPU | 264 MHz + 528 MHz
Memory (RAM) Capacity | 1,024 MB
Host Interface | USB interface: Hi-Speed USB x 4 (Front side x 1, Back side x 3) Network interface: Common to 10BASE-T/100BASE-TX/1000BASE-T (RJ-45) Full Duplex/Half Duplex
User Interface | LCD: 132 x 65 dots F-STN LCD LED indicator: 5 indicators Operation key: 12 keys Numeric key: Yes
ROM connector | 1 connector
SD card slot | 1 slot

## Software Specifications

Built-in Control Command | PCL6, PostScript 3, UFR II, PDF, and XPS
Built-in Scalable Font | PCL: 93 Scalable fonts, 10 Bitmap fonts PS: 136 standard fonts
Printable Range | Printable Area
Network Interface | Supported protocol TCP/IP (Frame type: Ethernet II) SMB (option) Print application LPD RAW IPP/IPPS FTP WSD

101K-07L