# Optional Items

The functionality of the machine can be fully utilized by using the optional items described below. Optional items can be purchased from the retail outlet where you purchased the machine or from your local Canon dealer.

### Paper Feeder PF-D1

|  | Use of the optional paper feeder allows you to load a different size of paper than that loadable in the standard paper drawer, thus reducing the time and labor of paper size replacement.

Available Paper | Paper
Power Supply | From main unit
Dimensions (W x L x H) | 458 x 464 x 150 mm
Weight | Approx. 6.1 kg

##### Installation Method

See "Getting Started."

You can install up to three units of paper feeder in LBP712Cx, and one unit in LBP710Cx.

### Barcode Printing Kit-F1

|  | If the Barcode Printing Kit-F1 is installed on the machine, barcode printing mode is added, enabling barcodes to be printed from your computer. The Barcode Printing Kit-F1 contains the following barcode fonts. OCR-B Symb. FontInform Symbole stethos BarDIMM ©1997 USPS ZEBRA+4Stat
|  | This option enables you to generate barcodes in various formats. Note that if you want to print barcodes, PCL must be enabled. For information on using the Barcode Printing Kit, see the Barcode Printing Guide (PDF manual). The Barcode Printing Guide is stored in the following folder on the Instruction Manual DVD-ROM. [LBP712C_710C Manual_ene]-[pdfs]-[Barcode Printing Guide]

##### Installation Method

Installing the ROM

### PCL International Font Set-C1

|  | If the PCL International Font Set-C1 is installed on the machine, the following fonts are added for a PCL printer. As a result, you can output using multiple languages in a SAP Unicode environment. Andale® and WorldType® Collection J (Japanese Version) Andale® and WorldType® Collection K (Korean Version) Andale® and WorldType® Collection S (Simplified Chinese Version) Andale® and WorldType® Collection T (Traditional Chinese Version) In order to support differences in character design depending on the region, four font versions are enabled.

##### Installation Method

Installing the ROM

### SD CARD-C1

|  | You can install the SD card to use the functions described below. Secured Print Printing a Document Secured by a PIN (Secured Print) Stored Job Print Printing a Document Stored in the Machine (Stored Job Print) Interrupt Print, Priority Print, Pause/Resume Checking Current Status of Print Documents SMB Print Configuring SMB Spooler Spooler

##### Installation Method

Installing an SD Card

When you dispose of a used SD card, perform <Completely Del. Data> for it or physically destroy it to prevent your personal information from being leaked. Installing an SD Card

101K-07W