# Interior

#### Toner cartridge slots

Load the toner cartridges in these slots: Y (yellow) in the leftmost slot, followed by M (magenta), C (cyan), and K (black). How to Replace Toner Cartridges

#### Delivery unit

If there is a paper jam inside the machine, raise the transport guide to remove the jammed paper. Clearing Jams

#### Transport guide

If paper has jammed inside the machine, lift up the delivery unit and open this guide to remove the jammed paper. Clearing Jams
101K-00A