# Memory Lock Settings

Normally, received documents are immediately printed. However, you can specify whether or not to store received faxes in memory before printing. You can then print the stored faxes at any time or delete them without printing to save paper.

###### How to access the option:

[] (Menu) -> <System Settings> -> <Communication Management Settings> -> <Memory Lock Settings>

| If <Memory Lock PIN> is specified, use the numeric keys [] to [] to enter those numbers, and then press [OK].

###### Settings:

(Bold: Default setting)

Off | Disable Memory Lock.
On | Memory Lock PIN: Seven-digit number | Once the PIN is set, you are prompted to enter it every time you change or disable the Memory Lock mode settings.
Report Print: Off, On | Specify whether to print the RX result report when receiving a fax. Activate "Receive Results Report" to enable this setting.
Memory Lock Time: Off, On | When <On> is set, received faxes are stored in memory only for a specified length of time. Set <Memory Lock Start Time> and <Memory Lock End Time> respectively.

NOTE
###### Memory Lock PIN: Press [OK] without entering any numbers when you do not want to set the PIN. You cannot set a PIN consisting only of <0> (<0000000>). ###### Memory Lock Settings operations: When memory lock settings are changed from <On> to <Off>, the documents saved in the memory up to then are combined and printed. "Combining and Printing the Received Documents You Saved" At <Memory Lock End Time>, you can combine and print received documents saved in the memory from the <Memory Lock Start Time> to the <Memory Lock End Time>.

0AE3-07C