# Miscellaneous Problems

###### See the following sections:

Steam is Emitted from the Machine's Output Area.
Water Droplets From on the Back Side of the Operation Panel and in the Output Area.
The Machine Makes a Clicking Sound.
The Settings That You Specified Are Not Enabled or Saved.

## Steam is Emitted from the Machine's Output Area.

Use only dry paper in the machine. Moisture evaporates from damp paper due to the heat generated inside the fixing unit (it is most likely to occur at low room temperatures). This is not a malfunction, but you can prevent this by using a stack of new unopened paper. However, if you smell something burning, immediately turn OFF the machine, unplug the power plug from the AC power outlet, and contact your local authorized Canon dealer or the Canon help line. Continued use may lead to a fire or electrical shock.

## Water Droplets From on the Back Side of the Operation Panel and in the Output Area.

Use only dry paper in the machine. Moisture evaporates from damp paper due to the heat generated inside the fixing unit (it is most likely to occur at low room temperatures). This is not a malfunction, but you can prevent this by using a stack of new unopened paper. However, if you smell something burning, immediately turn OFF the machine, unplug the power plug from the AC power outlet, and contact your local authorized Canon dealer or the Canon help line. Continued use may lead to a fire or electrical shock.

## The Machine Makes a Clicking Sound.

Make sure that the telephone cable is correctly connected. Make sure that the cables connected to the telephone line port and external device port on the back of the machine are not reversed. "Turning On the Machine and Specifying the Initial Settings"

## The Settings That You Specified Are Not Enabled or Saved.

If you turn OFF the machine immediately after changing settings via the operation panel, the settings may not be stored in the machine. After changing the settings, wait for approximately five seconds before turning OFF the machine.

0AE3-0C4