# Copy Specifications

Copy Specifications
Scan Resolution | Text/Photo(High Speed): 300 dpi x 300 dpi Text/Photo, Photo, Text: 600 dpi x 600 dpi
Maximum Scanning Size | Platen glass: 8 1/2" x 11 3/4" (215.9 mm x 297 mm) Feeder: 8 1/2" x 14" (216 mm x 356 mm)
Output Resolution | 600 dpi x 600 dpi
Copy Ratio | 100% Direct, 400% Max, 200%, 129% STMT->LTR, 78% LGL->LTR, 64% LTR->STMT, 50%, 25% Min
Copy Speed (Letter Plain Direct)* | 26 cpm
Continuous Copying Capacity | Maximum 99 copies
First Copy Time (Letter) | 8.7 seconds or less

* | The copy speed on Letter size plain paper on one-side printing is measured during continuous copying. Copy speeds vary depending on the output resolution, the paper type and size, and the paper feeding direction. Copy speeds on smaller paper sizes may be slower. Plus, the machine may experience downtime or decrease the copy speed in the middle of a continuous copy run to adjust the temperature inside the machine or maintain the optimal print quality.

0AE3-040