# Loading Small Size Paper In the Paper Cassette

Before loading paper in the paper cassette, see "Attention (Loading Paper)."

This section describes how to load small size paper in the paper cassette.
1
Open the front cover and the lower front cover.
2
Spread the paper guides a little wider than the paper size.

| If you want to change the size of the paper to be loaded, be sure to register the paper size in "Setting the Paper Size and Type."

3
Gently load the paper into the paper cassette with the print side face up, until the edge of the paper stack meets the back of the paper cassette.
"Paper Loading Capacity"
"Paper Loading Orientation"
Ensure that the paper stack does not exceed the load limit guides (A).
4
Adjust the paper guides tightly to the width of the paper.
5
Pick up the small paper guide from the paper cassette.
6
Attach the small paper guide to the paper guide and lower the small paper guide as shown below.
7
Adjust the paper guide tightly to the length of the paper.

IMPORTANT
###### Adjust the paper guides to the paper width without space. If the paper guides are loose or tight, this may result in misfeeds or paper jams.

8
Close the front cover and the lower front cover.
9
Lift the paper stopper.
10
Specify the loaded paper size and type.
"Setting the Paper Size and Type"
0AE3-02A