# Attention (Cleaning the Machine)

See "Maintenance and Inspections" in "Important Safety Instructions."

Before cleaning the machine, note the following:
Make sure that no jobs are stored in memory before turning OFF the power switch and disconnecting the power cord.
Use a soft cloth to avoid scratching the components.
Do not clean the machine components with tissue paper, paper towels, or similar materials. These materials tend to stick to the components or generate static charges.

CAUTION
###### Precautions to take when cleaning the feeder: Do not dampen the cloth too much, as this may tear the document or damage the machine. ###### Precautions to take when closing the feeder: Keep your fingers clear of the feeder to avoid injury. ###### Do not touch the fixing unit (A). Touching the fixing unit (A) may cause burns as it becomes very hot during use. ###### Precautions to take when you get toner onto your hands or into clothing: If toner comes in contact with your hands or clothing, wash them immediately in cold water. Do not use warm water, as it will set the toner and make it difficult to remove the toner stains.

IMPORTANT
###### Do not touch the transfer roller (A). Touching the transfer roller (A) may damage the machine.

NOTE
###### Sending or receiving faxes: When the power plug is unplugged, the machine cannot send or receive faxes.
###### When a job is waiting to be printed: The job is deleted when you turn OFF the power switch.
###### Jobs stored in memory: Jobs can be stored in memory even when the power plug has been unplugged. To view jobs stored in memory, see the following. "Managing Faxes Stored in Memory"

0AE3-0E2