# Launching SMS (Log in)

The following two methods are used for launching SMS.
Launching SMS directly from the Web browser
Launching SMS from a Remote UI

Before launching SMS, see "Attention (Launching SMS (Log in))."

## Launching SMS directly from the Web browser

1
Start the Web browser.
2
Enter "https://<Printer's IP address>:8443/sms/" in the address bar, and press [ENTER] from the Enter key on the keyboard.
Entry Example: https://192.168.0.215:8443/sms/

| If the printer's host name is registered in the DNS server, you can enter [host name.domain name] instead of the IP address. Input Example: http://my_printer.xy_dept.company.com:8443/sms/

If SMS does not launch Check the following. HTTP communication is enabled. "Setting Up HTTP Communication" The computer and printer are connected properly over the network. The printer is turned ON. The IP address or [host name.domain name] are entered correctly.

NOTE
###### Device Serial Number The printer's device serial number is displayed on the upper left of the screen. (The device serial number is required to obtain the license file from the license management system.)

3
Enter the password, and click [Login].

| The default password is "MeapSmsLogin" (case sensitive).

If you cannot log in If you cannot log in because the password is not correct, a message is displayed prompting you to re-enter your password. Enter the correct password, and click [Login].
| If you do not log in within approximately 5 minutes after the login page is displayed, you will not be able to log in even if you enter the correct password.
| A switch license file is required to initialize passwords. After clicking on [Browse] in [Initialize Password] in the screen that displays the message prompting password re-entry, select Switch License File, and click [Initialize]. Contact your local authorized Canon dealer or sales representatives.

## Launching SMS from a Remote UI

1
Start the Remote UI and log on in system manager mode.
"Starting the Remote UI"
2
Click [Service Management Service] on the portal page.
3
Enter the password, and click [Login].

| The default password is "MeapSmsLogin" (case sensitive).

If you cannot log in If you cannot log in because the password is not correct, a message is displayed prompting you to re-enter your password. Enter the correct password, and click [Login].
| If you do not log in within approximately 5 minutes after the login page is displayed, you will not be able to log in even if you enter the correct password.
| A switch license file is required to initialize passwords. After clicking on [Browse] in [Initialize Password] in the screen that displays the message prompting password re-entry, select Switch License File, and click [Initialize]. Contact your local authorized Canon dealer or sales representatives.

0258-0HA