# Clearing Paper Jams (Multi-purpose Tray)

Referring to the procedure on the display, follow the steps below to remove jammed documents.
1
Press [ ].
2
Remove the paper by pulling it gently.

###### If the jammed paper cannot be removed easily

Do not try to remove it forcefully but proceed to Step 3.
3
Close the multi-purpose tray.
4
Pull out the drawer.
5
Lower the manual feed transport guide.

(1) | Hold the tabs (A) on both sides.
(2) | Push them down.

IMPORTANT
###### Do not touch the rubber pad (A). Touching it may result in deterioration in print quality.

6
Remove the paper by pulling it gently.

###### If the jammed paper cannot be removed easily

Do not try to remove it forcefully but proceed to Step 7.
7
Return the manual feed transport guide to its original position.
8
Insert the drawer in the printer.
9
When the following screen appears, press [OK].
The machine is ready to print.

If the screen does not appear Open or close the front cover.

NOTE
###### If the jammed paper cannot be removed in Step 6 See "Clearing Paper Jams (Back Cover)" and remove the jammed paper.

Next, proceed to the clearing procedure for another area which is displayed in the message.
| (1) "Clearing Paper Jams (Multi-purpose Tray)"
| (2) "Clearing Paper Jams (Paper Drawer)"
| (3) "Clearing Paper Jams (Back Cover)"
| (4) "Clearing Paper Jams (Output Area)"

0258-0C4