# [Setup] Menu ([Paper Source] Options)

NOTE
###### Table description Bold values in the table indicate the default settings. The setting items or setting values with "*" may not be displayed depending on the availability of the optional accessories and other settings. ###### About the icons
: | The settings for the printer driver are prioritized for this item.
: | When you are printing from DOS, UNIX, or other operating systems which do not use the printer driver, the settings are enabled for this item.

Setting Item | Setting Value | Setting
[Paper Source] | [Auto], [Drawer 1], [Drawer 2]*, [Multi-Purpose Tray] | Select the default paper source that is used when printing.
[MP Tray Paper Size] | [A5], [B5], [A4], [LTR], [LGL], [EXEC], [Mixed Sizes], [Custom Size], [Custom Size R], [Env. ISO-C5], [Env. Monarch], [Env. No.10], [Env. DL], [Env. ISO-B5], [Index Card], [STMT], [FLSC] | Specifies the size of the paper loaded in the multi-purpose tray. "Registering the Paper Size and Type"
[MP Tray Priority] | [Off], [On] | Specifies whether the printer should detect the paper source in order starting with the multi-purpose tray when [Paper Source] is set to [Auto] in "[Select Feeder] Menu."
[Drawer 1 Size]/[Drawer 2 Size]* | [A5], [B5], [A4], [LTR], [LGL], [EXEC], [Mixed Sizes], [Custom Size], [Custom Size R], [Env. ISO-C5], [Env. No.10], [Env. DL], [Env. ISO-B5], [STMT], [FLSC] | Specifies the size of the paper loaded in the paper drawer. "Registering the Paper Size and Type"
[Standard Paper Size] | [A5], [B5], [A4], [LTR], [LGL], [EXEC], [Env. ISO-C5], [Env. Monarch], [Env. No.10], [Env. DL], [Env. ISO-B5], [Index Card], [STMT], [FLSC] | If you cannot specify the paper size or if you print from DOS, UNIX, or other operating system, specify the paper size in this item. "Loading Paper in the Drawer" "Loading Paper in the Multi-purpose Tray"
[Diff. Paper Tray] | [Off], [On] | Specifies whether the printer should feed paper from the multi-purpose tray when paper of the size for the received data is not loaded in the paper drawer.
[Auto Selection] | [Multi-Purpose Tray]: [Off], [On] [Drawer 1]: [Off], [On] [Drawer 2]*: [Off], [On] | Specifies the paper source to be automatically selected when [Paper Source] is set to [Auto] in "[Select Feeder] Menu." If [On] is specified, the printer selects the paper source as the one to be automatically selected.
[Default Paper Type] | [Plain], [Plain L], [Plain L2], [Plain H], [Heavy 1], [Heavy 2], [Heavy 3], [Transparency], [Envelope], [Envelope H], [Coated 1], [Coated 2], [Coated 3], [Coated 4], [Labels] | If you cannot specify the paper type or if you print from DOS, UNIX, or other operating system, specify the paper type in this item.
[MP Tray Paper Type] | [Plain], [Plain L], [Plain L2], [Plain H], [Heavy 1], [Heavy 2], [Heavy 3], [Transparency], [Envelope], [Envelope H], [Coated 1], [Coated 2], [Coated 3], [Coated 4], [Labels], [Mixed Types] | Set the type of paper that is loaded in the multi-purpose tray. "Registering the Paper Size and Type" "Usable Paper"
[Drawer 1 Type]/[Drawer 2 Type]* | [Plain], [Plain L], [Plain L2], [Plain H], [Heavy 1], [Heavy 2], [Heavy 3], [Envelope], [Envelope H], [Coated 1], [Coated 2], [Coated 3], [Coated 4], [Labels], [Mixed Types] | Set the type of paper that is loaded in the paper drawer. "Registering the Paper Size and Type" "Usable Paper"
[Manual 2-Sided (MP)] | [1st Side], [2nd Side] | Set the printing side of the paper that is loaded in the multi-purpose tray manually for 2-sided printing. When it is set to [1st Side], it is printed on the front of the paper (the side that is first be printed). When it is set to [2nd Side], it is printed on the back of the paper (the reverse side of the paper that has already been printed).
[2-Sided Printing] | [Off], [On] | Specifies whether the printer should print on one side or both sides of the paper.

0258-08R