# Square Areas That Cannot Be Seen on the Display Appear around Lines or Text and Are Printed in a Different Color from the Other Areas

Perform the following procedure.

#### <Cause> A process that is different from the specified halftone process or color process may be applied depending on the operating system or application.

Solution 1 | Perform the following procedure in the printer driver. UFR II Printer Driver
1. | Display the [Quality] sheet.
2. | Click [Advanced Settings].
3. | Set [Gray Compensation] to [All] or [Disabled].
PCL Printer Driver See Help of the PCL printer driver. You can specify the same setting from the printer's control panel. "[Setup] Menu ([Quality] Options)"
Solution 2 | Perform the following procedure in the printer driver. UFR II Printer Driver
1. | Display the [Quality] sheet.
2. | Click [Advanced Settings].
3. | Set [Halftones] to [Resolution] or [Gradation].
PCL Printer Driver See Help of the PCL printer driver. You can specify the same setting from the printer's control panel. "[Setup] Menu ([Quality] Options)"
Solution 3 | Perform the following procedure in the printer driver. UFR II Printer Driver
1. | Display the [Quality] sheet.
2. | Select the [Manual Color Settings] check box.
3. | Click [Color Settings].
4. | Display the [Matching] sheet.
5. | Set [Matching Method] for [Text], [Graphics], and [Images] to the same settings.
PCL Printer Driver See Help of the PCL printer driver. You can specify the same setting from the printer's control panel. "[Setup] Menu ([Quality] Options)"

0258-0R5