# The Print Server for Connection Cannot Be Found

Perform one of the following solutions according to the cause.

#### <Cause 1> The LAN cable is not connected properly.

Solution | Connect the print server to the client computer with the LAN cable properly.

#### <Cause 2> The print server has not been started up.

Solution | Start up the print server.

#### <Cause 3> The printer is not specified as a shared printer.

Solution | Specify the printer as a shared printer. For details, see the following item in "Printer Driver Installation Guide." "Installation" - "Print Server Settings" For details on the procedure for viewing "Printer Driver Installation Guide", see "Installation."

#### <Cause 4> The user does not have permission to access the print server or printer.

Solution | Ask your network administrator to change the user permissions.

#### <Cause 5> [Network discovery] is not enabled. (Windows Vista, 7, and Server 2008)

Solution | Perform either of the following procedures.
1. | From the [Start] menu, select [Control Panel].
2. | Click [View network status and tasks].
3. | Set [Network discovery] to [On].
1. | From the [Start] menu, select [Control Panel].
2. | Click [View network status and tasks].
3. | Click [Change advanced sharing settings].
4. | Specify [Turn on network discovery] in [Network discovery].
1. | From the [Start] menu, select [Control Panel].
2. | Double-click [Network and Sharing Center].
3. | Set [Network discovery] to [On].

0258-0AH