# The Overall Print Result Is Faint

Perform one of the following solutions according to the cause.

#### <Cause 1> The setting for the toner density is not appropriate.

Solution | Adjust the toner density for printing to a darker setting. "[Setup] Menu ([Quality] Options)"

#### <Cause 2> [Toner Save] is enabled.

Solution | UFR II Printer Driver Perform the following procedure in the printer driver.
1. | Display the [Quality] sheet.
2. | Click [Advanced Settings].
3. | Set [Toner Save] to [Off].
PCL/PS Printer Driver See Help of the PCL/PS printer driver. You can specify the same setting from the printer's control panel. "[Setup] Menu ([Quality] Options)"

0258-0E2