# Paper Loading and Output

This printer has the following paper sources and output trays.

Paper Source | (A): Multi-purpose tray | "Loading Paper in the Multi-purpose Tray"
(B): Drawer 1 | "Loading Paper in the Drawer"
(C): Drawer 2 (optional)
Output Tray | (D): Output tray | Outputs paper with the printed side facing down.

## Precautions for Output Trays

Pay attention to the following points when handling the output trays.

See "Important Safety Instructions" also.

During 2-sided printing, do not touch the paper until it is output to the output tray completely. The paper is first output partially after the front side is printed, and then it is fed again to be printed on the reverse side.

## Paper Capacity of the Paper Sources and Output Trays

: Unavailable

Paper Type | Paper Source | Output Tray
Multi-purpose tray | Drawer 1 | Drawer 2 (optional)
Plain paper (90 g/m²) | Approx. 50 sheets | Approx. 250 sheets | Approx. 250 sheets | Approx. 150 sheets
Heavy paper (120 g/m²) | Approx. 30 sheets | Approx. 200 sheets | Approx. 200 sheets | Approx. 50 sheets
Heavy paper (176 g/m²) | Approx. 20 sheets | Approx. 150 sheets | Approx. 150 sheets | Approx. 50 sheets
Transparency | Approx. 20 sheets |  |  | Approx. 10 sheets
Label | Approx. 20 sheets | Approx. 50 sheets | Approx. 50 sheets | Approx. 10 sheets
Envelope | Approx. 5 sheets | Approx. 10 sheets | Approx. 10 sheets | Approx. 10 sheets
Coated paper | Approx. 20 sheets | Approx. 50 sheets | Approx. 50 sheets | Approx. 50 sheets

* | Actual paper capacity varies depending on the installation environment, paper type or paper size to be used.

0258-033